>> MIB - Management Information Base
>> Table: mpsSysConfig - (.1.3.6.1.4.1.272.4.53.1.1)
mpsSysConfig
OID | Name | Type | Access
.1 | Country | ENUM | RW
.2 | SetExchangeDate | ENUM | RW
.3 | Facilities | BITS | RW
.4 | AreaCode | DisplayString | RW
.5 | CountryCode | DisplayString | RW
.6 | CodeInternationalPrefix | DisplayString | RW
.7 | CodeNationalPrefix | DisplayString | RW
.8 | CityCode | DisplayString | RW
.9 | Language | ENUM | RW
.10 | DefaultTargetType | ENUM | RW
.11 | DefaultTargetIndex | INTEGER | RW
.12 | ExtMoHVolume | INTEGER | RW
.13 | PreselectionCode | DisplayString | RW
Country
This variable contains the country code settings of the PBX, e.g. change CLIP information at calls to exter, change impedance settings at internal analogue ports. Enumerations: germany (1) netherlands (2) united-kindom (3) belgium (4) italy (5) denmark (6) spain (7) sweden (8) norway (9) france (10) portugal (11) austria (12) switzerland (13) czech (14) slovenia (15) poland (16) hungary (17) greece (18)
SetExchangeDate
Accept time and date is off, acceppt from exchange or accept from time server. Enumerations: no (1) pbx (2) time-server (3)
Facilities
System facilities: highRingerFrequency: a/b extension ringing frequency (0=50 Hz, 1=25 Hz) handoverBusyExtension: This value determines if handover to busy extension is possible handoverBusyMusicOnHold:This value determines if the caller hears tone or MoH connExtExt: Two external subscribers are to be connected after hang up. Enumerations: highRingerFrequency (0) handoverBusyExtension (1) handoverBusyMusicOnHold (2) connExtExt (3)
AreaCode
This variable contains the digits for the area code (national number, e.g. '5171'). Length: 0 to 10
CountryCode
This variable contains the digits for the country code (international number, e.g '49'). Length: 0 to 6
CodeInternationalPrefix
This variable contains the digits for international prefix code. Length: 0 to 2
CodeNationalPrefix
This variable contains the digit for national prefix code. Length: 0 to 1
CityCode
This variable contains the digit for the city code prefix. Extension with dial authorisation = 'local' can only dial numbers with this prefix. Length: 0 to 8
Language
This variable contains the language code setting, e.g for system provided menue. Enumerations: german (1) english (3) italian (5)
DefaultTargetType
This variable contains the default target type of system, if no incoming external call distribution match. 'off' means busy signalling to external subscriber. Enumerations: group (1) extension (2) none (3)
DefaultTargetIndex
This variable contains index of the target table or zero (busy signalling), mpsSysConfigDefaultTargetType=group : index = mpsGroupIndex. mpsSysConfigDefaultTargetType=extension : index = ExtensionIndex. Range: 0 to 65535
ExtMoHVolume
This variable contains the volume adjustment level for the external MoH played back via the audio-in jack (approximately in 3 dB steps): negative values -> attenuate during playback 0 -> original playback positive values -> amplify during playback Range: -5 to 3
PreselectionCode
This variable contains the digits for system preselection (call-by-call). Length: 0 to 10

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH