>> MIB - Management Information Base
>> Table: dot11MultiDomainCapabilityTable - (.1.2.840.10036.1.7.1)
Description: An entry (conceptual row) in the Multiple Domain Capability Table. IfIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB are indexed by ifIndex.
dot11MultiDomainCapabilityTable
OID | Name | Type | Access
.1 | MultiDomainCapabilityIndex | Integer32 | R
.2 | FirstChannelNumber | Integer32 | RW
.3 | NumberofChannels | Integer32 | RW
.4 | MaximumTransmitPowerLevel | Integer32 | RW
MultiDomainCapabilityIndex
The auxiliary variable used to identify instances of the columnar objects in the Multi Domain Capability Table. Range: 1 to 2147483647
FirstChannelNumber
This attribute shall indicate the value of the lowest channel number in the subband for the associated domain country string. The default value of this attribute shall be zero.
NumberofChannels
This attribute shall indicate the value of the total number of channels allowed in the subband for the associated domain country string. The default value of this attribute shall be zero.
MaximumTransmitPowerLevel
This attribute shall indicate the maximum transmit power, in dBm, allowed in the subband for the associated domain country string. The default value of this attribute shall be zero.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH