>> MIB - Management Information Base
>> Table: biboPingTable - (.1.3.6.1.4.1.272.4.5.27.1.1)
Description: Contains parameters for the ping and results of the operation. To create a new entry, do an SNMP SET request including a biboPingIndex value which is not in use. To delete an existing entry, do an SNMP SET request including a biboPingStatus value equal to delete (6).
biboPingTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Status | ENUM | D
.3 | Completed | ENUM | R
.4 | SourceAddress | IpAddress | RW
.5 | Address | IpAddress | RW
.6 | PacketCount | INTEGER | RW
.7 | PacketSize | INTEGER | RW
.8 | PacketTimeout | INTEGER | RW
.9 | ReceivedPackets | INTEGER | R
.10 | MinRoundTrip | INTEGER | R
.11 | MaxRoundTrip | INTEGER | R
.12 | AvgRoundTrip | INTEGER | R
.13 | TTL | INTEGER | RW
.14 | TOS | INTEGER | RW
Index
The unique index of the entry. Range: 1 to 2147483647
Status
The current status of the entry or a request to discard it (delete). Enumerations: active (1) notinservice (2) notready (3) createandgo (4) createandwait (5) delete (6)
Completed
The completion status of the ping session. Enumerations: true (1) false (2)
SourceAddress
The source ip-address for the ping session.
Address
The target ip-address for the ping session.
PacketCount
The number of ping packets to send. 0 means continuous send. Range: 0 to 65535
PacketSize
The size of each ping packet in bytes. Range: 8 to 4096
PacketTimeout
The amount of time in milliseconds to wait for a reply before deciding the packet is lost. Range: 1 to 65535
ReceivedPackets
The number of replies received so far. Range: 0 to 65535
MinRoundTrip
The minimum round trip time in milliseconds for all the packets which have been replied to. Range: 0 to 65535
MaxRoundTrip
The maximum round trip time in milliseconds for all the packets which have been replied to. Range: 0 to 65535
AvgRoundTrip
The average round trip time in milliseconds for all the packets which have been replied to. Range: 0 to 65535
TTL
The TTL byte value for each packet (0 = IP default). Range: 0 to 255
TOS
The TOS byte value for each packet. Range: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH