>> MIB - Management Information Base
>> Table: localUdpLimitTable - (.1.3.6.1.4.1.272.4.5.14.4.1)
Description: Table to be used to limit access to local UDP services.
localUdpLimitTable
OID | Name | Type | Access
.1 | AdminState | ENUM | D
.2 | Service | ENUM | RW
.3 | MaxRate | INTEGER | RW
.4 | CurRate | Counter | R
.5 | State | ENUM | R
AdminState
The administrative state of this limit entry. Enumerations: active (1) inactive (2) delete (3)
Service
The corresponding UDP service. Enumerations: snmp (1) rip (2) bootps (3) dns (4) nbns (5) statmon (6)
MaxRate
Maximum number of packets per second for this UDP service. Range: 0 to 65536
CurRate
The current number of packets per second for this UDP service.
State
The current state for this UDP service. Enumerations: below (1) exceeded (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH