>> MIB - Management Information Base
>> Table: biboAdmLicenseTable - (.1.3.6.1.4.1.272.254.4.1)
Description: This table contains the licenses, purchased for this BIANCA/BRICK. Each entry describes a license. Each license can enable one or more features of the BIANCA/BRICK, when the activation key is correct. Please Note, that a license is only valid for the BIANCA/BRICK it has been purchased for.
biboAdmLicenseTable
OID | Name | Type | Access
.1 | SerialNumber | INTEGER | RW
.2 | Mask | INTEGER | RW
.3 | Key | DisplayString | RW
.4 | State | ENUM | D
.5 | SerialId | DisplayString | RW
.6 | HwSerial | DisplayString | R
.7 | LicType | ENUM | R
SerialNumber
This object specifies the serial number of the license in case of a numerical license (together with 'Mask' and 'Key'). Range: 0 to 999999
Mask
The LicenseMask is a bitfield, that specifies the different features enabled by the license. (only used on a numerical license). Range: 0 to 8388607
Key
This object contains the activation key. A license is only valid, if the activation key is correct. Length: 0 to 255
State
To delete a license from the system, this object has to be set to delete. In case of an 'internal-ok' license the license can be erased from the modules EEPROM, if it is set to 'internal-erase'. The state will be 'not-supported' if a license refers to a feature which is not supported by the image loaded. With 'delete' it is only deleted from the main board flash memory. Enumerations: ok (1) not-ok (2) delete (3) internal-ok (4) internal-erase (5) not-supported (6)
SerialId
This object specifies the serial id string of the license in case of string license (together with 'Key'). Length: 0 to 255
HwSerial
This object contains the device Hardware serial number for which the license is purchased for. Length: 0 to 255
LicType
The type of licenseable feature. Enumerations: ip (1) capi (2) bridge (3) x25 (4) ipx (5) stac (6) frame-relay (7) tapi (8) ospf (9) extended-lan (10) tunneling (11) taf (12) extended-wan (13) leased-line (14) e25 (29) ipsec (33) ipseccb-ipxfer (34) bgp (35) uefs (36) siplan (37) siptrunk (38) pim (39) call-by-call (40) fax (41) sipout (42) brrp (43) wlan-controller (44) terminal-option (45) data-encr-accel (46) voice-mail-system (47) pptp (48) ethernet (128) bri (129) g703 (130) pri (131) modem (132) g7032pri (133) slots (134) e3 (135) serial (136) shdsl (137) vdsl (138)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH