>> MIB - Management Information Base
>> Table: wlcVSSProfileTable - (.1.3.6.1.4.1.272.4.61.1.20.1)
Description: This table contains different VSS setting profiles.
wlcVSSProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Id | DisplayString | RW
.3 | Name | DisplayString | RW
.4 | AdminStatus | ENUM | D
.5 | Security | ENUM | RW
.6 | DefaultKey | ENUM | RW
.7 | Key1 | OCTET STRING | RW
.8 | Key2 | OCTET STRING | RW
.9 | Key3 | OCTET STRING | RW
.10 | Key4 | OCTET STRING | RW
.11 | Total | INTEGER | RW
.12 | MAC | ENUM | RW
.13 | Local | ENUM | RW
.14 | Hidden | ENUM | RW
.15 | WPAUnicastCipher | BITS | RW
.16 | RSNUnicastCipher | BITS | RW
.17 | WpaMixedMode | ENUM | RW
.18 | RsnPreauthentication | ENUM | RW
.19 | WMM | ENUM | RW
.20 | ARPProcessing | ENUM | RW
.21 | VlanId | INTEGER | RW
.22 | SoftTotal | INTEGER | RW
.23 | BandSteeringPreference | ENUM | RW
.24 | Blacklist | ENUM | RW
.25 | UAPSD | ENUM | RW
.26 | StaRxShaping | INTEGER | RW
.27 | StaTxShaping | INTEGER | RW
Index
Unique VSS profile index.
Id
This attribute reflects the Service Set ID used in the DesiredSSID parameter of the most recent MLME scan request. Length: 0 to 32
Name
The VSS profile name. Length: 0 to 255
AdminStatus
Enable, disable or delete the requested VSS profile. Enumerations: disabled (1) enabled (2) delete (32)
Security
The Security Option which will be used. wep40 and wep104:= WEP-Authentication wpa-psk := WPA-Authentication with PSK wpa := WPA-Authentication with radius (802.1X) wpa2 := OBSOLETE and not used anymore! Enumerations: none (1) wep40 (2) wep104 (3) wpa-psk (4) wpa (5) wpa2 (6)
DefaultKey
Default key for WEP encryption. Enumerations: key1 (1) key2 (2) key3 (3) key4 (4)
Key1
Key string for WEP key no. 1. Also used for WPA passphrase. Length: 0 to 64
Key2
Key string for WEP key no. 2. Length: 0 to 64
Key3
Key string for WEP key no. 3. Length: 0 to 64
Key4
Key string for WEP key no. 4. Length: 0 to 64
Total
The number of allowed clients of the requested VSS. Range: 1 to 256
MAC
MAC Media Access Control via MAC Address. Enumerations: true (1) false (2)
Local
Routing between connected Clients. Enumerations: true (1) false (2)
Hidden
Define whether SSID is hidden (true) or not (false). Default value is false. Enumerations: true (1) false (2)
WPAUnicastCipher
The set of unicast ciphers used for WPA. Enumerations: tkip (1) aes (2)
RSNUnicastCipher
The set of unicast ciphers used for RSN. Enumerations: tkip (1) aes (2)
WpaMixedMode
Allows mixed operation of WPA and WPA2 by value wpaandwpa2(3) (default value). For tightened security, value wpa2(2) can be selected. The value wpa(1) is available for some older clients with drivers that are unable to deal with WPA2 information elements. Enumerations: wpa (1) wpa2 (2) wpaandwpa2 (3)
RsnPreauthentication
When this object is set to TRUE, this shall indicate that RSNA preauthentication is enabled on this entity. This object requires that dot11RSNAEnabled also be set to TRUE. Enumerations: true (1) false (2)
WMM
This object defines whether WMM (Wi-Fi Multimedia) is active for this service set. Depending on the WLAN hardware and driver, WMM might only be allowed for one service set, i.e. enabling WMM for one service set disables WMM for all other service sets. Enumerations: true (1) false (2)
ARPProcessing
This object defines whether ARP processing is active for this service set or not. ARP processing is a feature to reduce the number of ARP broadcast packets. If the AP finds the requested IP address in the node table it exchanges the broadcast MAC address by the unicast MAC address of the client. Default is false. Enumerations: true (1) false (2)
VlanId
The VLAN-Tag-Id used for the virtual interface. Range: 0 to 4095
SoftTotal
If wlcVSSProfileSoftTotal STAs are connected to this VSS, subsequent association attempts will be rejected with BUSY. If a STA still tries to associate within 30sec, the association request will be accepted. Range: 1 to 256
BandSteeringPreference
Define the preferred band for Band Steering. none : no preference (default) b24-GHz: prefer 2,4 GHz b5-GHz : prefer 5 GHz Enumerations: none (1) bs-24GHz (2) bs-5GHz (3)
Blacklist
Enable or disable blacklisting via MAC addresses. Enumerations: enable (1) disable (2)
UAPSD
Enable or disable UAPSD Enumerations: enable (1) disable (2)
StaRxShaping
STA to AP bandwidth limitation per associated station. The value is given in bits per seconds, -1 is unlimited (default)
StaTxShaping
AP to STA bandwidth limitation per associated station. The value is given in bits per seconds, -1 is unlimited (default)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH