>> MIB - Management Information Base
>> Table: mediaTerminalTable - (.1.3.6.1.4.1.272.4.50.2.1)
Description: Definition of a NAT access rules to a SIP terminal (device) located in LAN.
mediaTerminalTable
OID | Name | Type | Access
.1 | IntAddr | IpAddress | RW
.2 | IntPort | INTEGER | RW
.3 | ExtPort | INTEGER | RW
.4 | RemotePort | INTEGER | RW
.5 | Lifetime | INTEGER | RW
.6 | Age | INTEGER | R
.7 | Proto | ENUM | RW
.8 | Type | ENUM | D
.10 | Sessions | INTEGER | R
IntAddr
The terminal's internal address (address of a device in LAN).
IntPort
The terminal's internal port (port of a device in LAN). Range: 0 to 65535
ExtPort
The terminal's external port (a port on the WAN side of the gateway used for NAT access to a device in LAN). Range: 0 to 65535
RemotePort
The port of a remote device (located in WAN): this entry is only useful for 'Type' = 'client'. In all other cases this value has to be '0' (disabled). Range: 0 to 65535
Lifetime
The lifetime of sessions (s) defined by this terminal entry: this parameter is only useful for 'Type' = 'client'. In this case 'Lifetime' is set to 86400 seconds by default. So if the terminal did not send or receive any data within this timeout, this terminal entry will be deleted. For 'Type' = 'server' the lifetime has to be '0' (disabled).
Age
Current age of terminal's last action.
Proto
The terminal's transport protocol: 'udp' -> terminal uses UDP as transport; 'tcp' -> terminal uses TCP as transport. Default value is udp. Enumerations: tcp (6) udp (17)
Type
The type of the terminal entry: 'client' -> autodetected (and thus listed here automatically) or manually added IP phone or softclient; 'server' -> manually added internal rerouted SIP server; 'delete' -> delete flag. Manually added clients are usually obsolete as they are autodetected by the Application Level Gateway anyways (see ipProxyTable for definition of dynamic NAT rules). 'Type' = 'server' is used in order to enable access from WAN to a SIP registrar or SIP proxy located in LAN. Enumerations: client (1) server (2) delete (8)
Sessions
Terminal's currently active RTP sessions.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH