>> MIB - Management Information Base
>> Table: localUdpAllowTable - (.1.3.6.1.4.1.272.4.5.14.2.1)
Description: Filter rule table for incoming UDP packets for local services. This table is used to restrict access to UDP services provided by the system. o active rules have at least one of 'localUdpAllowAddrMode' and 'localUdpAllowIfMode' set to 'verify' o if there are active rules for a certain service, incoming packets of this service type must match at least one of them. o incoming packets to a service (port) without an active rule are always allowed. o packets originating from 127.0.0.1 are always allowed
localUdpAllowTable
OID | Name | Type | Access
.1 | AddrMode | ENUM | D
.2 | Addr | IpAddress | RW
.3 | Mask | IpAddress | RW
.4 | IfMode | ENUM | RW
.5 | IfIndex | INTEGER | RW
.6 | Service | ENUM | RW
AddrMode
Specifies wether or not the IP source address of incoming UDP packets should be checked against localUdpAllowAddr and localUdpAllowMask. Enumerations: dont-verify (1) verify (2) delete (3)
Addr
Check source IP address against contents of this variable, taking localUdpAllowMask into account.
Mask
Specifies address mask to use for IP source address comparisson with address contained in localUdpAllowAddr.
IfMode
Specifies wether or not the source interface of incoming UDP packets should checked Enumerations: dont-verify (1) verify (2)
IfIndex
Specifies source interface index for interface check in case localUdpAllowIfMode is set to verify.
Service
service Enumerations: snmp (1) rip (2) bootps (3) dns (4) nbns (5) statmon (6)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH