>> MIB - Management Information Base
>> Table: l2tpGlobals - (.1.3.6.1.4.1.272.4.23.8.10)
l2tpGlobals
OID | Name | Type | Access
.10 | UdpPort | INTEGER | RW
.20 | PortUsage | ENUM | RW
UdpPort
The UDP port which is monitored by L2TP for tunnel establishment requests received from remote hosts. Range: 1 to 65535
PortUsage
This object specifies whether L2TP uses only one UDP port (which number is defined by l2tpGlobUdpPort), or if it allocates a new available port, to send messages to the remote equipment. Choosing 'single' makes it sometimes easier to process L2TP through NAT since L2TP traffic can be classified based on the UDP port number. Choosing 'floating' selects the behavior which is recommended in RFC2331. Possible values: single(1), -- L2TP uses the UDP port defined by l2tpGlobUdpPort -- to send messages to the remote equipment. floating(2) -- L2TP allocates a new port to send messages to -- the remote equipment (default). Enumerations: single (1) floating (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH