>> MIB - Management Information Base
>> Table: usbEndpointDescTable - (.1.3.6.1.4.1.272.4.55.4.1)
Description: (one entry of usbEndpointDescEntry)
usbEndpointDescTable
OID | Name | Type | Access
.1 | DescDevAddr | INTEGER | R
.2 | DescIfcIndex | INTEGER | R
.3 | DescIfcNum | INTEGER | R
.4 | DescEpAddress | INTEGER | R
.5 | DescPipeDirection | ENUM | R
.6 | DescPipeType | ENUM | R
.7 | DescAttributes | INTEGER | R
.8 | DescMaxPacketSize | INTEGER | R
.9 | DescInterval | INTEGER | R
.10 | DescRawData | OCTET STRING | R
.11 | StatXferPackets | Counter32 | R
.12 | StatXferBytes | Counter32 | R
.13 | StatXferQlen | Counter32 | R
.14 | StatXferStalled | Counter32 | R
.15 | StatXferIoError | Counter32 | R
.16 | StatXferBabble | Counter32 | R
.17 | StatXferOverrun | Counter32 | R
.18 | StatXferToggle | Counter32 | R
DescDevAddr
DevAddr = (slot << 12) | (unit << 8) | (Enum << 4) | IfcNum. Enum is assigned by the USB device enumerator. Range: 0 to 65535
DescIfcIndex
Index = PipeType << 5 | PipeDirection << 4 | EpAddress. Used for unique enumeration of the endpoints. Range: 0 to 255
DescIfcNum
The interface number of the endpoints interface. Range: 0 to 255
DescEpAddress
The endpoints address (direction bit stripped). Range: 0 to 15
DescPipeDirection
Transfer direction of this endpoint. Enumerations: in (1) out (2)
DescPipeType
The endpoint type extracted from the endpoint descriptor attribute field. Enumerations: ctrl (1) iso (2) bulk (3) intr (4)
DescAttributes
Complete endpoint atribute field. For debugging only. Range: 0 to 255
DescMaxPacketSize
The maximum packet size the endpoint is capable of sending or receiving. Range: 0 to 65535
DescInterval
Interval for polling endpoint data transfers (in frame counts). Ignored for bulk and control endpoints. Iso endpoints must be equal 1. Field may range from 1 to 255 for interrupt endpoints. Range: 0 to 255
DescRawData
Endpoint descriptor raw data for debugging purposes only. Length: 0 to 7
StatXferPackets
The number of packets transferred by the endpoint.
StatXferBytes
The number of bytes transferred by the endpoint.
StatXferQlen
The number of frames enqueued at the endpoint.
StatXferStalled
The number of stall conditions detected.
StatXferIoError
The number of I/O errors detected.
StatXferBabble
The number of Babble errors detected.
StatXferOverrun
The number of Frame Overrun errors detected.
StatXferToggle
The number of Toggle errors detected.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH