>> MIB - Management Information Base
>> Table: mpsCallThroughTable - (.1.3.6.1.4.1.272.4.53.4.5.1)
Description: This table contains the information about call through handling.
mpsCallThroughTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | InTrunkGroup | TrunkGroupIndex | RW
.3 | InNumberIndex | TrunkNumberIndex | RW
.4 | OutTrunkGroup | TrunkGroupIndex | RW
.5 | OutNumberIndex | TrunkNumberIndex | RW
.6 | OutBundle | Unsigned32 | RW
.7 | Facilities | BITS | R
.8 | AdminStatus | ENUM | D
.9 | Option | ENUM | RW
.10 | Extension | ExtensionIndexOrZero | RW
.11 | PIN | DisplayString | RW
Index
A unique value for each call through entry.
InTrunkGroup
A unique value for the incoming trunk group. Reference to mpsTrunkGroupTable. Range: 1 to 65535
InNumberIndex
This value index of the incoming external MSN. Reference to mpsTrunkNumberTable. Range: 1 to 65535
OutTrunkGroup
A unique value for the outgoing trunk group. Reference to mpsTrunkGroupTable. Range: 1 to 65535
OutNumberIndex
This value index of the outgoing external MSN. Reference to mpsTrunkNumberTable. Range: 1 to 65535
OutBundle
A unique value for the outgoing bundle. Reference to mpsTrunkBundleTable.
Facilities
Special facilities of the call through entry. clip_sreening : sreen the incoming phone number. ars : use ars (automatic route selection) Enumerations: clip-sreening (0) ars (1)
AdminStatus
For enable, disable or delete. Enumerations: enable (1) disable (2) delete (3)
Option
This variable contains the authorisation option for the calling party. clipscr -> only CLIP screening pin -> only PIN check clipscrAndPin -> CLIP screening and PIN check clipscrOrPin -> CLIP screening or PIN check Enumerations: clipscr (1) pin (2) clipscrAndPin (3) clipscrOrPin (4)
Extension
This variable contains the extension for outgoing call routing. Range: 0 to 65535
PIN
This variable contains the PIN code for call through, if set in mpsCallThroughOption. Length: 6 to 6

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH