>> MIB - Management Information Base
>> Table: systemPhoneMSNTable - (.1.3.6.1.4.1.272.4.64.1.4.1)
Description: This table contains configuration data assigned to a specific MSN of the system phone.
systemPhoneMSNTable
OID | Name | Type | Access
.1 | ExtTermIndex | SystelExtTerminalIndex | RW
.2 | MelodyExt | INTEGER | RW
.3 | VolumeExt | INTEGER | RW
.4 | MelodyInt | INTEGER | RW
.5 | VolumeInt | INTEGER | RW
.6 | CfNumber | DisplayString | RW
.7 | CdNumber | DisplayString | RW
.8 | AdminStatus | ENUM | D
ExtTermIndex
A reference to the mpsExtensionTerminalTable. Range: 1 to 65535
MelodyExt
The variable contains the number index of a specific melody for signalling external calls. This melody is generated within the system phone. Range: 0 to 19
VolumeExt
Volume of the external ringing melody: 0..6: Muted .. Loud 7: Increasing volume. NG system phones have different ranges of values: 1..9: Soft .. Loud 10: Increasing volume. Range: 0 to 10
MelodyInt
The variable contains the number index of a specific melody for signalling internal calls. This melody is generated within the system phone. Range: 0 to 19
VolumeInt
Volume of the internal ringing melody: 0..6: Muted .. Loud 7: Increasing volume. NG system phones have different ranges of values: 1..9: Soft .. Loud 10: Increasing volume. Range: 0 to 10
CfNumber
Number of a call forwarding target, specific for this MSN. Length: 0 to 26
CdNumber
Number of a call deflection target, specific for this MSN. Length: 0 to 26
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH