>> MIB - Management Information Base
>> Table: wlcVSSTable - (.1.3.6.1.4.1.272.4.61.1.19.1)
Description: This table combines WTP with the VSS profile.
wlcVSSTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | wlanIfIndex | INTEGER | RW
.3 | ProfIndex | INTEGER | RW
.4 | AdminStatus | ENUM | D
Index
This variable contains a unique index.
wlanIfIndex
This variable is the WLAN interface of the requested WTP WLAN interface.
ProfIndex
This variable contains the unique VSS profile index.
AdminStatus
Enable or delete the VSS profile from the requested WTP. Enumerations: disabled (1) enabled (2) default (3) delete (32)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH