>> MIB - Management Information Base
>> Table: wlanScanResultsTable - (.1.3.6.1.4.1.272.4.46.15.1)
Description: This table contains the list of BSS entries found by foreground or background scanning in client mode.
wlanScanResultsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Index | INTEGER | R
.3 | BSSID | MacAddress | R
.4 | Age | INTEGER | R
.5 | RSSI | WlanRSSI | R
.6 | SSID | DisplayString | R
.7 | Channel | INTEGER | R
.8 | DTIMPeriod | INTEGER | R
.9 | BeaconPeriod | INTEGER | R
.10 | CapInfo | INTEGER | R
.11 | Rates | OCTET STRING | R
.12 | BasicRates | OCTET STRING | R
.13 | ExtendedRates | OCTET STRING | R
.14 | FrameData | OCTET STRING | R
.15 | Type | ENUM | R
.16 | Privacy | ENUM | R
.17 | WPAUnicastCipher | BITS | R
.18 | RSNUnicastCipher | BITS | R
.19 | RSSI1 | WlanRSSI | R
.20 | RSSI2 | WlanRSSI | R
.21 | RSSI3 | WlanRSSI | R
.22 | FirstSeen | Date | R
.23 | LastSeen | Date | R
.24 | Signal | WlanRSSI | R
.25 | WPAMulticastCipher | ENUM | R
.26 | RSNMulticastCipher | ENUM | R
IfIndex
ifIndex of the WLAN Interface the scan results belong to.
Index
Auxiliary index for different BSS entries.
BSSID
BSSID of this BSS. Length: 6 to 6
Age
Age of this BSS entry.
RSSI
Receive signal strength of this BSS. Range: -110 to 0
SSID
SSID aka network name of this BSS. If broadcasting of SSID is disabled on this BSS, this string may be empty. Length: 0 to 255
Channel
The channel this BSS was received on. Range: 1 to 256
DTIMPeriod
The number of DTIM intervals between the start of CFPs for this BSS. Range: 0 to 255
BeaconPeriod
This attribute contains the number of TU that this BSS uses for scheduling Beacon transmissions. Range: 1 to 65535
CapInfo
The number of DTIM intervals between the start of CFPs for this BSS.
Rates
This attribute contains one octet for each supported rate in this BSS, in 500 Kbps units.
BasicRates
This attribute contains one octet for each required basic rate in this BSS, in 500 Kbps units.
ExtendedRates
This attribute contains one octet for each supported extended rate in this BSS, in 500 Kbps units.
FrameData
This attribute contains raw data from 802.11 beacon or probe response frames, starting with the 802.11 timestamp.
Type
This attribute contains the device type of the scanned device. Enumerations: access-point (1) ad-hoc (2)
Privacy
This attribute contains the privacy type of the scanned device. Enumerations: none (1) wep (2) wpa-psk (3) wpaandwpa2-psk (4) wpa2-psk (5) wpa-enterprise (6) wpaandwpa2-enterprise (7) wpa2-enterprise (8)
WPAUnicastCipher
This attribute contains the WPA unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4)
RSNUnicastCipher
This attribute contains the RSN unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4)
RSSI1
Receive signal strength of this BSS at first receiver. Range: -110 to 0
RSSI2
Receive signal strength of this BSS at second receiver. A value of 0 indicates no second receiver present. Range: -110 to 0
RSSI3
Receive signal strength of this BSS at third receiver. A value of 0 indicates no third receiver present. Range: -110 to 0
FirstSeen
The timestamp, when this known AP was first seen.
LastSeen
The timestamp, when this AP was last seen.
Signal
Receive signal strength of this BSS. Range: -110 to 0
WPAMulticastCipher
This attribute contains the WPA multicast cipher of the scanned AP.
RSNMulticastCipher
This attribute contains the RSN multicast cipher of the scanned AP.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH