>> MIB - Management Information Base
>> Table: layer25BridgeTable - (.1.3.6.1.4.1.272.4.56.2.1)
Description: Each entry consists of a unique IP address and corresponding layer-2 informations.
layer25BridgeTable
OID | Name | Type | Access
.1 | IpAddr | IpAddress | R
.2 | MacAddr | MacAddress | R
.3 | PortIfIndex | INTEGER | R
.4 | LinkIfIndex | INTEGER | R
IpAddr
The IP address identifying the host on layer-3.
MacAddr
The MAC address identifying the host on layer-2. Length: 6 to 6
PortIfIndex
The layer-2 port over which the host is currently reachable.
LinkIfIndex
The bridge group the host logically belongs to.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH