>> MIB - Management Information Base
>> Table: auxStatTable - (.1.3.6.1.4.1.272.4.41.3.1.11.1)
Description: A single auxStatTable entry.
auxStatTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | OperStatus | ENUM | R
.3 | ErrorCode | ENUM | R
.4 | Network | DisplayString | R
.5 | Command | DisplayString | R
.6 | Answer | DisplayString | R
.7 | CSQ | INTEGER | R
.8 | ControlChannel | ENUM | R
.9 | AccessType | ENUM | R
.10 | InDiscards | INTEGER | R
.11 | HomePLMN | INTEGER | R
.12 | CurrentPLMN | INTEGER | R
.13 | IMEI | DisplayString | R
.14 | IccId | DisplayString | R
.15 | LocationAreaCode | DisplayString | R
.16 | CellId | DisplayString | R
IfIndex
The index of the corresponding tty interface.
OperStatus
The operational status of the GSM modem. The following states can occur: - up(1) the device is up - initialization finished - down(2) the device is down - init(3) initialization state - called(4) incoming call received - calling(5) dialout is performed - connect(6) connection established - simwait(7) modem is detected - SIM card not ready - pinwait(8) modem is waiting for non-empty PIN entry - error(9) error - for details consult ErrorCode - disconnected(10) the device isn't available (unplugged) - pukwait(11) waiting for PUK entry after PIN invalidated - regwait(12) wating for network operator registration - apnwait(13) waiting for APN entry if APN is empty The initial OperStatus is down(2). Enumerations: up (1) down (2) init (3) called (4) calling (5) connect (6) simwait (7) pinwait (8) error (9) disconnected (10) pukwait (11) regwait (12) apnwait (13)
ErrorCode
If an error occurs (OperStatus is set to error) this variable shows the reason for the error. Currently the following error codes are possible: - none(1) no error occured - unspecified(2) error can't be specified any further - pinerror(3) PIN was wrong PUK needed - pukerror(4) PUK was wrong - apnerror(5) APN was wrong - simerror(6) SIM card not present or damaged - reg-denied(7) Network registration denied The initial ErrorCode is none(1). Enumerations: none (1) unspecified (2) pinerror (3) pukerror (4) apnerror (5) simerror (6) reg-denied (7)
Network
The name of the PLMN (Public Land Mobile Network) actually being used. Length: 0 to 60
Command
The last Command that was sent to the Modem. Length: 0 to 40
Answer
The last Answer gotten from the Modem. Length: 0 to 60
CSQ
The GSM receive signal level in decibel (db). A value below -100 signals a very low signal quality. A value between -100 and -80 means that signal quality is low. If the value is between -80 and -70 the quality is ok. The interval from -70 to -60 signals a good quality and if the value is above -60 the quality is excellent. The default e.g. initial value is -113.
ControlChannel
If the UMTS card provides several channels and one could be used to control the card e.g. get status information from the card like the signal quality a dedicated daemon will do this and the auxStatControlChannel will be set to available. In the other case auxStatControlChannel is set to not_available. Enumerations: not-available (1) available (2)
AccessType
The Access Type the modem actually registers on. Normally the `edge' or `hs*pa' Access Types aren't provided in detail by the operator. Enumerations: unknown (1) gsm (2) compact-gsm (3) umts (4) gsm-edge (5) umts-hsdpa (6) umts-hsupa (7) umts-hspa (8)
InDiscards
The number of frames which can't be enqueued upstream.
HomePLMN
The PLMN (Public Land Mobile Network) code of the Home PLMN.
CurrentPLMN
The PLMN (Public Land Mobile Network) code of the Network currently used.
IMEI
The IMEI (International Mobile Equipment Identity) of the detected GSM/UMTS device. Length: 0 to 32
IccId
The ICC-ID of the SIM-Card found in the device which is actually enumerated with auxStatIfIndex. Some UMTS modem vendors offer no capability to read this ID before entering a valid PIN :-( In this case the default configuration is choosen. Length: 0 to 32
LocationAreaCode
The actual Location Area Code the UMTS-Modem is registered. This may differ for GSM/UMTS Access Technology. Length: 0 to 16
CellId
The actual Cell-ID the UMTS-Modem is registered. This may differ for GSM/UMTS Access Technology. Length: 0 to 16

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH