>> MIB - Management Information Base
>> Table: dot11SupportedMCSRxTable - (.1.2.840.10036.4.17.1)
Description: An Entry (conceptual row) in the dot11SupportedMCSRx Table. ifIndex - Each IEEE 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11SupportedMCSRxTable
OID | Name | Type | Access
.1 | Index | Integer32 | R
.2 | Value | Integer32 | R
Index
Index object that identifies which MCS to access. Range is 1..255. Range: 1 to 255
Value
The receive MCS supported by the PLCP and PMD, represented by a count from 1 to 127, subject to limitations of each individual PHY. Range: 1 to 127

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH