>> MIB - Management Information Base
>> Table: ipHostsAliveTable - (.1.3.6.1.4.1.272.4.5.19.1)
Description: This table specifies the watched IP addresses. Entries in the table are created and removed manually by network management.
ipHostsAliveTable
OID | Name | Type | Access
.1 | Group | INTEGER | RW
.2 | IPAddress | IpAddress | RW
.3 | State | ENUM | R
.4 | Interval | INTEGER | RW
.5 | DownAction | ENUM | D
.6 | FirstIfIndex | INTEGER | RW
.7 | Range | INTEGER | RW
.8 | SrcIPAddress | IpAddress | RW
.9 | Trials | INTEGER | RW
.10 | Backups | INTEGER | RW
Group
The group of the watched IP-Addresses Range: 0 to 255
IPAddress
The watched IP-Address. If set to zero, the default gateway is used.
State
The State of the watched IP-Address Enumerations: alive (1) down (2)
Interval
This is the time interval for state verification Range: 1 to 65536
DownAction
Action be performed if the ipHostsAliveState changes to down (2), If set to none (4) there is no action specified, if set to monitor (7) this entry just enables monitoring of this status in other subsystem context like IP load balancing. Enumerations: up (1) down (2) delete (3) none (4) reset (5) redial (6) monitor (7)
FirstIfIndex
The first ifc
Range
The range of all ifc's Range: 0 to 65536
SrcIPAddress
The source IP-Address
Trials
How many ping attempts until host is considered down. Default value is 3. Range: 1 to 65535
Backups
How many successful pings until host is considered up. Default value is 1. Range: 1 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH