>> MIB - Management Information Base
>> Table: dot11PhyAntennaTable - (.1.2.840.10036.4.2.1)
Description: An entry in the dot11PhyAntenna Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyAntennaTable
OID | Name | Type | Access
.1 | CurrentTxAntenna | Integer32 | RW
.2 | DiversitySupport | ENUM | R
.3 | CurrentRxAntenna | Integer32 | RW
.4 | AntennaSelectionOptionImplemented | ENUM | R
.5 | TransmitExplicitCSIFeedbackASOptionImplemented | ENUM | R
.6 | TransmitIndicesFeedbackASOptionImplemented | ENUM | R
.7 | ExplicitCSIFeedbackASOptionImplemented | ENUM | R
.8 | TransmitIndicesComputationFeedbackASOptionImplemented | ENUM | R
.9 | ReceiveAntennaSelectionOptionImplemented | ENUM | R
.10 | TransmitSoundingPPDUOptionImplemented | ENUM | R
CurrentTxAntenna
The current antenna being used to transmit. This value is one of the values appearing in dot11SupportedTxAntenna. This may be used by a management agent to control which antenna is used for transmission. Range: 1 to 255
DiversitySupport
This implementation's support for diversity, encoded as: X'01'-diversity is available and is performed over the fixed list of antennas defined in dot11DiversitySelectionRx. X'02'-diversity is not supported. X'03'-diversity is supported and control of diversity is also available, in which case the attribute dot11DiversitySelectionRx can be dynamically modified by the LME. Enumerations: fixedlist (1) notsupported (2) dynamic (3)
CurrentRxAntenna
The current antenna being used to receive, if the dot11 DiversitySupport indicates that diversity is not supported. The selected antenna shall be one of the antennae marked for receive in the dot11AntennasListTable. Range: 1 to 255
AntennaSelectionOptionImplemented
This attribute, when TRUE, indicates that antenna selection is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitExplicitCSIFeedbackASOptionImplemented
This attribute, when TRUE, indicates that the transmit Antenna Selection based on explicit CSI feedback is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitIndicesFeedbackASOptionImplemented
This attribute, when TRUE, indicates that the transmit antenna selection based on antenna indices feedback is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ExplicitCSIFeedbackASOptionImplemented
This attribute, when TRUE, indicates that the computation of CSI and feedback to support the peer to do antenna selection is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitIndicesComputationFeedbackASOptionImplemented
This attribute, when TRUE, indicates that the transmit antenna selection based on antenna indices selection computation and feedback the results to support the peer to do antenna selection is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ReceiveAntennaSelectionOptionImplemented
This attribute, when TRUE, indicates that the receive antenna selection is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitSoundingPPDUOptionImplemented
This attribute, when TRUE, indicates that the transmission of sounding PPDUs is supported by the station implementation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH