>> MIB - Management Information Base
>> Table: pppDialProfileTable - (.1.3.6.1.4.1.272.4.3.11.1)
Description: The pppDialProfileTable contains default parameters used for establishing dialout connections in cases where there is no partner specific configuration available (see biboDialTable). Creating entries: Entries are created by assigning a value to the pppDialProfileType object. Deleting entries: An entry can be removed by assigning the value `delete' to its pppDialProfileType object.
pppDialProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Descr | DisplayString | RW
.3 | BapNumber | DisplayString | RW
.4 | BapSubAddress | DisplayString | RW
.5 | BapLkType | ENUM | D
.6 | StkMask | BitValue | RW
.7 | CallbackL1Prot | ENUM | RW
Index
This object uniquely references this dialout profile. The index value is generated automatically.
Descr
A textual string describing this dialout profile. Length: 0 to 255
BapNumber
This object decribes the phone delta to use in a BAP Call-Response or Callback-Request according RFC 2125. Length: 0 to 63
BapSubAddress
This object decribes the subaddress to use in a BAP Call-Response or Callback-Request according RFC 2125. Length: 0 to 63
BapLkType
This object describes the link type to use in a BAP Call-Response or Callback-Request according RFC 2125. Enumerations: isdn (1) x25 (2) analog (3) isdn-dovb (5) delete (8)
StkMask
This binary number defines the ISDN stack(s) to use. Each bit corresponds to one entry (stack) in the isdnStkTable, the rightmost bit selects entry 0, the next bit selects entry 1, and so forth. For example, StkMask=0b1101 means: Allow to use ISDN stacks 0, 2and 3. A mask of 0 disables dialup completely, while a mask of -1 enables dialup on all available ISDN stacks. Range: 0 to -1
CallbackL1Prot
This entry is used to select the layer 1 protocol settings for callback. if set to initial(1), the selected layer 1 protocol of the initial call will be used to perform the callback. Enumerations: initial (1) data-64k (2) data-56k (3) modem (4) dovb (5) v110-1200 (6) v110-2400 (7) v110-4800 (8) v110-9600 (9) v110-14400 (10) v110-19200 (11) v110-38400 (12) modem-profile-1 (13) modem-profile-2 (14) modem-profile-3 (15) modem-profile-4 (16) modem-profile-5 (17) modem-profile-6 (18) modem-profile-7 (19) modem-profile-8 (20) pptp-pns (21) pppoe (22) aodi (23) pptp-pac (24) pppoa (25) l2tp-lac (26) pppox25 (27) dovb-64k (29) gprs (30)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH