>> MIB - Management Information Base
>> Table: tr069Admin - (.1.3.6.1.4.1.272.4.22.6.1)
tr069Admin
OID | Name | Type | Access
.1 | URL | DisplayString | RW
.2 | Username | DisplayString | RW
.3 | Password | DisplayString | RW
.4 | PeriodicInformEnable | ENUM | RW
.5 | PeriodicInformInterval | INTEGER | RW
.6 | PeriodicInformTime | INTEGER | RW
.8 | ConnectionRequestUsername | DisplayString | RW
.9 | ConnectionRequestPassword | DisplayString | RW
.10 | UpgradesManaged | ENUM | RW
.11 | Enabled | ENUM | RW
.12 | ACSAuthEnforced | ENUM | RW
.13 | ConnectionRequestPath | DisplayString | RW
.14 | DHCPURL | DisplayString | RW
.15 | CaCertIndex | INTEGER | RW
.16 | CertIndex | INTEGER | RW
URL
URL for the CPE to connect to the ACS using the CPE WAN Management Protocol. See TR-106 Amendment 2, Common Object Definitions: URL Length: 0 to 255
Username
Username used to authenticate the CPE when establishing a HTTP connection to the ACS using the CPE WAN management protocol. See TR-106 Am.2, Common Object Definitions: Username Length: 0 to 255
Password
Password used to authenticate the CPE when establishing a connection to the ACS. See TR-106 Am.2, Common Object Definitions: Password Length: 0 to 255
PeriodicInformEnable
If set to true, the CPE must periodically connect to the ACS server and send CPE information using the Inform method call. See TR-106 Am.2, Common Object Definitions: PeriodicInformEnable Enumerations: false (1) true (2)
PeriodicInformInterval
The duration in seconds of the interval for which the CPE MUST attempt to connect with the ACS and call the Inform method if PeriodicInform-Enable is true. See TR-106 Am.2, Common Object Definitions: PeriodicInformInterval Range: 1 to 2147483647
PeriodicInformTime
An absolute time reference in UTC to determine when the CPE should initiate the Inform method calls. Each inform call must occur at this reference time plus or minus an integer multiple of the PeriodicInformInterval. A zero value inidicates that no particular time reference is specified. That is, the CPE may locally choose the time referencer, required only to adhere to the specified PeriodicInformInterval. See TR-106 Amendment 2, Common Object Definitions: PeriodicInformInterval Currently not supported! Set only 0! Range: 0 to 2147483647
ConnectionRequestUsername
The username the ACS uses to authenticate itself to the CPE. See TR-106 Am.2, Common Object Definitions: ConnectionRequestUsername Length: 0 to 255
ConnectionRequestPassword
The password the ACS uses to authenticate itself to the CPE. See TR-106 Am.2, Common Object Definitions: ConnectionRequestPassword Length: 0 to 255
UpgradesManaged
Indicates whether or not the ACS will manage upgrades for the CPE. If true, the CPE SHOULD not use other means other than the ACS to seek out available upgrades. If false, the CPE MAY use other means for this purpose. Currently not supported, the CPE does not check for automatic upgrades. Enumerations: false (1) true (2)
Enabled
Global switch to enable or disable the TR-069 completely. Enumerations: false (1) true (2)
ACSAuthEnforced
If true and the ACS URL is https(SSL) the ACS must authenticate itself to the CPE. Enumerations: false (1) true (2)
ConnectionRequestPath
The path of the URL the ACS must access to request a connection. Length: 0 to 31
DHCPURL
If an ACS URL ist received via DHCP vendor option, it is stored here Length: 0 to 255
CaCertIndex
The index of the ca certificate to use (from the certTable).
CertIndex
The index of the certificate to use (from the certTable).

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH