>> MIB - Management Information Base
>> Table: pppPppoaPvcDevTable - (.1.3.6.1.4.1.272.4.3.18.1)
Description: .
pppPppoaPvcDevTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Index | INTEGER | RW
.10 | OperStatus | ENUM | R
.11 | ResidualBlockTime | INTEGER | R
IfIndex
The associated interface index of this entry.
AdminStatus
The administrative this entry. Enumerations: enabled (1) disabled (2) delete (3)
Index
Specifies the first device to be used for PPP over ATM (PPPoA) according RFC 2364.
OperStatus
The PPP-internal operational status of the first device to be used for PPP over ATM (PPPoA) according RFC 2364. Enumerations: dormant (1) connecting (2) up (3) blocked (4)
ResidualBlockTime
The remaining time interval till the associated pppPppoaPvcDevOperStatus will be changed from blocked(4) to dormant(1) again. Range: 0 to 2147483647

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH