>> MIB - Management Information Base
>> Table: ipsecTuning - (.1.3.6.1.4.1.272.4.26.32)
ipsecTuning
OID | Name | Type | Access
.1 | MaxPeers | INTEGER | R
.2 | PeerHashLines | INTEGER | RW
.3 | MaxTrafs | INTEGER | R
.4 | TrafHashLines | INTEGER | RW
.5 | SaBIDHashLines | INTEGER | RW
.6 | SAIHashLines | INTEGER | RW
.7 | TunRngHashLines | INTEGER | RW
.8 | BundleIdxHashLines | INTEGER | RW
.9 | IfcHashLines | INTEGER | RW
.10 | DevHashLines | INTEGER | RW
.11 | RtHashLines | INTEGER | RW
.12 | ExtRtHashLines | INTEGER | RW
.13 | MaxCacheEntries | INTEGER | RW
.14 | CacheHashLines | INTEGER | RW
.15 | MaxProfiles | INTEGER | R
.16 | IPFragMaxBytes | INTEGER | RW
.17 | IPFragMaxFragments | INTEGER | RW
.18 | IPFragMaxTraces | INTEGER | RW
.19 | AutoRehashMaxEntriesPerLine | INTEGER | RW
.20 | AutoRehashMaxRehashedEntriesPerLine | INTEGER | RW
MaxPeers
Maximum number of supported peers.
PeerHashLines
Number of peer hash lines (i.e. hash modulo).
MaxTrafs
Maximum number of supported traffic list entries.
TrafHashLines
Number of traffic hash lines (i.e. hash modulo).
SaBIDHashLines
Number of SA bundle ID hash lines (i.e. hash modulo).
SAIHashLines
Number of SA identifier hash lines (i.e. hash modulo).
TunRngHashLines
Number of tunnel range hash lines (i.e. hash modulo).
BundleIdxHashLines
Number of bundle index hash lines (i.e. hash modulo).
IfcHashLines
Number of interface hash lines (i.e. hash modulo).
DevHashLines
Number of device hash lines (i.e. hash modulo).
RtHashLines
Number of route hash lines (i.e. hash modulo).
ExtRtHashLines
Number of extended route hash lines (i.e. hash modulo).
MaxCacheEntries
Maximum number of cache entries allocated.
CacheHashLines
Number of cache hash lines (i.e. hash modulo).
MaxProfiles
Maximum number of supported ipsec profile list entries.
IPFragMaxBytes
Maximum number of bytes stored in fragments. Exceeding this limit results in discarding oldest trace(s).
IPFragMaxFragments
Maximum number of stored fragments. Exceeding this limit results in discarding oldest trace(s).
IPFragMaxTraces
Maximum number of traces. Exceeding this limit results in discarding oldest trace(s).
AutoRehashMaxEntriesPerLine
This variable defines the average number of entries per hash line, when rehashing is performed. A value of 4 means e.g., that when the number of entries in a hash table becomes four times the number of current anchors, a rehash is performed. Value 0 has the special meaning of turning off automatic rehashing, like negative values do. NOTE: automatic rehashing overwrites any specific fix settings! Default value is 4.
AutoRehashMaxRehashedEntriesPerLine
This variable defines the average number of entries per hash line, when rehashing is finished. A value of 2 means e.g., that, after rehashing finished, the number of entries in the hash table is at most twice the number of hash anchors (i.e. number of hash anchors increased accordingly). If the value is configured to be greater or equal to ipsecTuneAutoRehashMaxEntriesPerLine, automatic rehashing is de facto disabled, automatic decreasing of hash anchors isn't performed. Default value is 2.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH