>> MIB - Management Information Base
>> Table: capiApplTable - (.1.3.6.1.4.1.272.4.7.1.1)
Description: The capiApplTable contains information for all currently registered CAPI 1.1 and CAPI 2.0 applications, and their respective CAPI_REGISTER information. Creating entries: Entries are created automatically by the system. After receiving an appropriate CAPI_REGISTER call, the system 'registers' the application, and assigns it a unique capiApplNumber. Deleting entries: Once an application releases, entries are automatically removed by the system.
capiApplTable
OID | Name | Type | Access
.1 | Number | INTEGER | R
.2 | Version | ENUM | R
.3 | ByteOrder | ENUM | R
.4 | RegLevel3Cnt | INTEGER | R
.5 | RegMsgCnt | INTEGER | R
.6 | RegDblkCnt | INTEGER | R
.7 | RegDblkSize | INTEGER | R
.8 | InfoStr | DisplayString | R
Number
Identification number of the registered application.
Version
The version number of the registered application. Enumerations: capi11 (1) capi20 (2)
ByteOrder
The byte order used by the application. Enumerations: little-endian (1) big-endian (2) undef (3)
RegLevel3Cnt
CAPI_REGISTER: The number of level 3 connections this application accepts.
RegMsgCnt
CAPI_REGISTER: The number of registered CAPI messages this application accepts.
RegDblkCnt
CAPI_REGISTER: The number of registered B3 data blocks this application accepts.
RegDblkSize
CAPI_REGISTER: The size of registered B3 data blocks this application accepts.
InfoStr
Information string of CAPI instance: IP address and TCP port of connecting system and user name if any. Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH