>> MIB - Management Information Base
>> Table: biboBrrpOperTable - (.1.3.6.1.4.1.272.4.40.1.1)
Description: An entry in the biboBrrpOperTable containing the operational characteristics of a virtual router. On a BRRP router, a given virtual router is identified by a combination of the IF index and VRID. Rows in the table cannot be modified unless the value of `biboBrrpOperAdminState' is `disabled' and the `biboBrrpOperState' has transitioned to `initialize'.
biboBrrpOperTable
OID | Name | Type | Access
.1 | OperVrId | INTEGER | RW
.2 | VirtIfIndex | INTEGER | RW
.3 | OperMasterIpAddr | IpAddress | RW
.4 | OperState | ENUM | R
.5 | OperAdminState | ENUM | D
.6 | OperPriority | INTEGER | RW
.7 | OperAuthType | ENUM | RW
.8 | OperAuthKey | OCTET STRING | RW
.9 | OperAdvertisementInterval | INTEGER | RW
.10 | OperMasterDownRetries | INTEGER | RW
.11 | OperPreemptMode | ENUM | RW
.12 | OperVirtualRouterUpTime | TimeTicks | R
.14 | MasterIfIndex | INTEGER | RW
.15 | OperDecrPrio | INTEGER | R
OperVrId
This object contains the Virtual Router Identifier (VRID). Range: 1 to 255
VirtIfIndex
The index of the virtual interface used by the virtual router.
OperMasterIpAddr
The master router's real (primary) IP address. This is the IP address listed as the source in BRRP advertisement last received by this virtual router.
OperState
The current state of the virtual router. This object has four defined values: - `initialize', which indicates that all the virtual router is waiting for a startup event. - `backup', which indicates the virtual router is monitoring the availability of the master router. - `master', which indicates that the virtual router is forwarding packets for IP addresses that are associated with this router. Setting the `brrpOperAdminState' object (below) initiates transitions in the value of this object. Enumerations: initialize (1) backup (2) master (3)
OperAdminState
This object will enable/disable the virtual router function. Setting the value to `up', will transition the state of the virtual router from `initialize' to `backup' or `master', depending on the value of `brrpOperPriority'. Setting the value to `down', will transition the router from `master' or `backup' to `initialize'. State transitions may not be immediate; they sometimes depend on other factors, such as the interface (IF) state. The `brrpOperAdminState' object must be set to `down' prior to modifying the other read-only objects in the conceptual row. The value of the `brrpOperRowStatus' object (below) must be `active', signifying that the conceptual row is valid (i.e., the objects are correctly set), in order for this object to be set to `up'. Use `delete' to delete this table entry permanently. Enumerations: up (1) down (2) delete (3)
OperPriority
This object specifies the priority to be used for the virtual router master election process. Higher values imply higher priority. A priority of '0', although not settable, is sent by the master router to indicate that this router has ceased to participate in BRRP and a backup virtual router should transition to become a new master. A priority of 255 is used for the router that owns the associated IP address(es). Range: 1 to 255
OperAuthType
Authentication type used for BRRP protocol exchanges between virtual routers. This value of this object is the same for a given ifIndex. New enumerations to this list can only be added via a new RFC on the standards track. Enumerations: noAuthentication (1) simpleTextPassword (2) ipAuthenticationHeader (3)
OperAuthKey
The Authentication Key. This object is set according to the value of the 'brrpOperAuthType' object ('simpleTextPassword' or 'ipAuthenticationHeader'). If the length of the value is less than 16 octets, the agent will left adjust and zero fill to 16 octets. The value of this object is the same for a given ifIndex. When read, biboBrrpOperAuthKey always returns an Octet String of length zero. Length: 0 to 16
OperAdvertisementInterval
The time interval, in seconds, between sending advertisement messages. Only the master router sends BRRP advertisements. Range: 1 to 255
OperMasterDownRetries
Calculation of the MasterDownInterval from RFC 2338: Skew_Time = ((256 - Priority) / 256) MasterDownInterval = (MasterDownRetries * AdvertisementInterval) + Skew_Time Range: 1 to 255
OperPreemptMode
Controls whether a higher priority virtual router will preempt a lower priority master. Enumerations: false (1) true (2)
OperVirtualRouterUpTime
This is the value of the `sysUpTime' object when this virtual router (i.e., the `brrpOperState') transitioned out of `initialized'.
MasterIfIndex
The index of the master interface controlling the virtual router.
OperDecrPrio
This is the value currently decremented from the virtual router priority to be used for the virtual router master election process Actual priority = (biboBrrpOperPriority - biboBrrpOperDecrPrio) This value could be either '0' or 'aliveSlaveBrrpDecrPrio': - it is set to 'aliveSlaveBrrpDecrPrio' when the alive surveillance (aliveSlaveBrrpState) triggers 'decrPrio' while this router state is 'up' (biboBrrpOperState). - it is cleared to '0' when the alive surveillance (aliveSlaveBrrpState) triggers 'up' while this router state is already 'up' (biboBrrpOperState). The default value is '0'. Range: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH