>> MIB - Management Information Base
>> Table: msdp - (.1.3.6.1.4.1.272.4.5.56.1.1)
msdp
OID | Name | Type | Access
.1 | Enabled | ENUM | RW
.2 | CacheLifetime | TimeTicks | RW
.3 | NumSACacheEntries | Gauge32 | R
.4 | RPAddress | IpAddress | RW
Enabled
The state of MSDP on this MSDP speaker - globally enabled or disabled. Changes to this object should be stored to non-volatile memory. Enumerations: true (1) false (2)
CacheLifetime
The lifetime given to SA cache entries when created or refreshed in seconds. This is the [SG-State-Period] in the MSDP spec.
NumSACacheEntries
The total number of entries in the SA Cache table.
RPAddress
The Rendezvous Point (RP) address used when sourcing MSDP SA messages. May be 0.0.0.0 on non-RPs. Changes to this object should be stored to non-volatile memory.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH