>> MIB - Management Information Base
>> Table: dot11PhyHRDSSSTable - (.1.2.840.10036.4.12.1)
Description: An entry in the dot11PhyHRDSSSEntry Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyHRDSSSTable
OID | Name | Type | Access
.3 | ChannelAgilityPresent | ENUM | R
.4 | ChannelAgilityEnabled | ENUM | R
.5 | HRCCAModeSupported | INTEGER | R
.16 | ShortPreambleOptionImplemented | ENUM | R
.27 | PBCCOptionImplemented | ENUM | R
ChannelAgilityPresent
This attribute indicates that the PHY is capable of channel agility. Enumerations: true (1) false (2)
ChannelAgilityEnabled
This attribute indicates that the PHY channel agility functionality is enabled. Enumerations: true (1) false (2)
HRCCAModeSupported
dot11HRCCAModeSupported is a bit-significant value, representing all of the CCA modes supported by the PHY. Valid values are: energy detect only (ED_ONLY) = 01, carrier sense only (CS_ONLY) = 02, carrier sense and energy detect (ED_and_CS)= 04 carrier sense with timer (CS_and_Timer)= 08 high rate carrier sense and energy detect (HRCS_and_ED)= 16 or the logical sum of any of these values. In the high rate extension PHY, this attribute shall be used in preference to the dot11CCAModeSupported attribute. Range: 1 to 31
ShortPreambleOptionImplemented
This attribute, when true, shall indicate that the short preamble option as defined in subclause 18.2.2.2 is implemented. The default value of this attribute shall be false. Enumerations: true (1) false (2)
PBCCOptionImplemented
This attribute, when true, shall indicate that the PBCC modulation option as defined in subclause 18.4.6.6 is implemented. The default value of this attribute shall be false. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH