>> MIB - Management Information Base
>> Table: usbDeviceDescTable - (.1.3.6.1.4.1.272.4.55.1.1)
Description: (one entry of usbDeviceDescTable)
usbDeviceDescTable
OID | Name | Type | Access
.1 | DevAddr | INTEGER | R
.2 | UpTime | TimeStamp | R
.3 | Status | ENUM | R
.4 | BcdUSB | ENUM | R
.5 | DeviceClass | ENUM | R
.6 | DeviceSubClass | INTEGER | R
.7 | DeviceProtocol | INTEGER | R
.8 | MaxPacketSize | INTEGER | R
.9 | IdVendor | INTEGER | R
.10 | IdProduct | INTEGER | R
.11 | BcdDevice | INTEGER | R
.12 | TxtManufacturer | DisplayString | R
.13 | TxtProduct | DisplayString | R
.14 | TxtSerialNumber | DisplayString | R
.15 | NumConfigurations | INTEGER | R
.16 | RawData | OCTET STRING | R
.17 | HubPortNumber | INTEGER | R
.18 | DeviceSpeed | ENUM | R
.19 | Depth | INTEGER | R
.20 | Parent | INTEGER | R
DevAddr
DevAddr = (slot << 12) | (unit << 8) | (Enum << 4). Enum is assigned by the USB device enumerator. Range: 0 to 65535
UpTime
TimeStamp when the USB host controller/root hub detected the inserted USB device.
Status
Current status of the USB device: attach - attach the device to the specified device class config - configure the device if supported detach - detach the device from upper layers. Enumerations: attach (1) config (2) detach (3)
BcdUSB
The USB standard supported by the device. Enumerations: unspecified (1) usb1-0 (2) usb1-1 (3) usb2-0 (4) usb3-0 (5)
DeviceClass
The class code of the USB device. 0x00 - each interface specifies it's own class code. 0xFF - the class code is vendor specific. Otherwise the value is a valid class code. Enumerations: spec-in-ifc (0) comm (2) hub (9) diagnostic (220) wireless (224) vendor-spec (255)
DeviceSubClass
DeviceClass dependent SubClass code. There are no unique values over all DeviceClasses defined. Range: 0 to 255
DeviceProtocol
DeviceClass and SubClass dependent DeviceProtocol code. There are no unique values over all DeviceClasses defined. Range: 0 to 255
MaxPacketSize
The maximum packet size supported by the USB device. This value normally depends on the USB standard supported. Range: 0 to 255
IdVendor
The unique USB device vendor ID. Range: 0 to 65535
IdProduct
The (hopefully) unique USB device product ID. Range: 0 to 65535
BcdDevice
The USB device release number in BCD format. Range: 0 to 65535
TxtManufacturer
Human readable manufacturers name (if present). Length: 0 to 255
TxtProduct
Human readable product name (if present). Length: 0 to 255
TxtSerialNumber
Human readable serial number (if present). Length: 0 to 255
NumConfigurations
The number of alternative device configurations supported by the USB device. Range: 0 to 255
RawData
Device descriptor raw data for debugging purposes only. Length: 0 to 18
HubPortNumber
The number of the port the USB device is connected to. Range: 0 to 15
DeviceSpeed
The speed the USB device uses for data transmission. Enumerations: low (1) full (2) high (3)
Depth
The depth in the bus topology where the device is located. 0 = Root Hub, 1 = Device at Root Hub, 2 = Device at ext. Hub, 3 = Device at external Hub connected to an external Hub, etc. Range: 0 to 7
Parent
DevAddr = (slot << 12) | (unit << 8) | (Enum << 4) of the parent hub for this device. Enum is assigned by the USB device enumerator. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH