>> MIB - Management Information Base
>> Table: mpsExtensionVoIPTable - (.1.3.6.1.4.1.272.4.53.6.6.1)
Description: This table contains additional information for VoIP extension.
mpsExtensionVoIPTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | Location | ENUM | RW
.3 | Network | NetworkIndex | RW
.4 | AdminStatus | ENUM | D
.5 | AdminBinding | DisplayString | RW
.6 | Facilities | BITS | RW
.7 | IpAddressInfo | IpAddress | R
.8 | OperationBinding | DisplayString | R
.9 | OperationStatus | ENUM | R
.10 | CurrentCalls | Counter32 | R
.11 | Codecs | BitValue | RW
.12 | CodecOrder | ENUM | RW
.13 | CodecProperties | CodecIndexOrZero | RW
Index
This variable references the mpsExtensionIndex. Range: 1 to 65535
Location
This variable contains the registration location area from which the subscriber is able to setup an VoIP-register. Enumerations: none (1) any (2) nowan (3) lan (4) wan (5) network (6)
Network
If mpsSubsRegistrationLocation = network (6), this value contains the special location index. Range: 1 to 18
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
AdminBinding
This variable contains name, port and transport of a statically registered client. example: 192.0.0.1:5060;tcp or phone30.bintec.de:5060;upd Data will be used, if mpsExtensionVoIPFacilities static is set. Length: 0 to 64
Facilities
Special facilities of the IP client. static: establish client with fix IP and port, no register possible. g726coding: 0 -> I.366 1 -> RFC 3551/X.420 no-auto-hold: allow multiple connections from this extension. srtp: allow SRTP negotiation no_holdretrieve: no hold and retrieve to sip phone public-registration: allow client registrations from public network. t38support: T.38 Fax signalling/coding allowed for this VoIP extension (disabled per default). Enumerations: static (0) g726coding (1) no-auto-hold (2) srtp (3) no-holdretrieve (4) public-registration (5) t38support (6)
IpAddressInfo
This variable contains the IP Address of the dynamically registered client, to show info in UI.
OperationBinding
This variable contains name:port of the registered client, to show info in UI. Length: 0 to 32
OperationStatus
This variable contains the actual operation status. notregistered : client is not registered registering : notregistered, registration pending registered : client is registered reregistering : registered, reregistration pending Enumerations: notregistered (1) registering (2) registered (3) reregistering (4)
CurrentCalls
This variable contains the current calls.
Codecs
For codecs, supported for this extension: ulaw (1) alaw (2) g729 (4) g726 (8) g726_16 (16) g726_32 (32) g726_40 (64) g728 (128) g723_63 (256) g723_53 (512) g729_e (1024) gsm (2048) dtmf (4096) Default ulaw, alaw, g.729 and dtmf Range: 0 to -1
CodecOrder
Sorting the codecs default -> system default order quality -> highest quality first lowest -> lowest bandwith first highest -> highest bandwith first Enumerations: default (1) quality (2) lowest (3) highest (4)
CodecProperties
A reference to mpsCodecPropertyTable for codec properties. 0 = use system default. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH