>> MIB - Management Information Base
>> Table: mpsFaxSwitchUserTable - (.1.3.6.1.4.1.272.4.53.11.3.1)
Description: This table contains the information about current mode for fax switches.
mpsFaxSwitchUserTable
OID | Name | Type | Access
.1 | Index | FaxSwitchIndex | RW
.2 | ModeNumber | FaxSwitchModeIndex | RW
.3 | AdminStatus | ENUM | D
Index
A unique value for each fax switch. Use the same value in mpsFaxSwitchIndex and mpsFaxSwitchModeIndex as reference to this entry. Range: 1 to 65535
ModeNumber
Select the active fax mode number. If a calendar in mpsFaxSwitchTable is selected the mode is switched automatically. Range: 1 to 2
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH