>> MIB - Management Information Base
>> Table: wlanWDSTable - (.1.3.6.1.4.1.272.4.46.3.1)
Description: WDS Link Configuration
wlanWDSTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | IfIndex | INTEGER | R
.3 | wlanIf | INTEGER | RC
.4 | AdminStatus | ENUM | D
.5 | Address | MacAddress | RC
.6 | PrivacyMode | ENUM | RC
.7 | PrivacyAutoKey | INTEGER | RC
.8 | LinkAliasName | OCTET STRING | RC
.9 | OperStatus | ENUM | R
.10 | DefaultKey | ENUM | RC
.11 | Key1 | OCTET STRING | RC
.12 | Key2 | OCTET STRING | RC
.13 | Key3 | OCTET STRING | RC
.14 | Key4 | OCTET STRING | RC
.15 | PassPhrase | OCTET STRING | RC
.17 | MSDUTx | Counter32 | R
.18 | MSDURx | Counter32 | R
.19 | BytesTx | Counter32 | R
.20 | BytesRx | Counter32 | R
.21 | CurrentRate | WlanRate | R
.22 | CurrentRSSI | WlanRSSI | R
.23 | CurrentNoise | WlanRSSI | R
.24 | TransientKey | OCTET STRING | N
.25 | LocalAddress | MacAddress | RC
.26 | TimeoutCount | Counter32 | N
.27 | RxFrames54 | Counter32 | R
.28 | RxFrames48 | Counter32 | R
.29 | RxFrames36 | Counter32 | R
.30 | RxFrames24 | Counter32 | R
.31 | RxFrames18 | Counter32 | R
.32 | RxFrames12 | Counter32 | R
.33 | RxFrames11 | Counter32 | R
.34 | RxFrames9 | Counter32 | R
.35 | RxFrames6 | Counter32 | R
.36 | RxFrames5 | Counter32 | R
.37 | RxFrames2 | Counter32 | R
.38 | RxFrames1 | Counter32 | R
.39 | TxFrames54 | Counter32 | R
.40 | TxFrames48 | Counter32 | R
.41 | TxFrames36 | Counter32 | R
.42 | TxFrames24 | Counter32 | R
.43 | TxFrames18 | Counter32 | R
.44 | TxFrames12 | Counter32 | R
.45 | TxFrames11 | Counter32 | R
.46 | TxFrames9 | Counter32 | R
.47 | TxFrames6 | Counter32 | R
.48 | TxFrames5 | Counter32 | R
.49 | TxFrames2 | Counter32 | R
.50 | TxFrames1 | Counter32 | R
.51 | CurrentRSSI1 | WlanRSSI | R
.52 | CurrentRSSI2 | WlanRSSI | R
.53 | CurrentRSSI3 | WlanRSSI | R
Index
Unique index of a WDS link Range: 0 to 31
IfIndex
IfIndex of the WDS.
wlanIf
IfIndex of the Interface the WDS belongs to.
AdminStatus
Enable or disable the requested WDS. Enumerations: enable (1) disable (2) delete (3)
Address
MAC Address of the WDS partner. Length: 6 to 6
PrivacyMode
This attribute selects privacy mode to use for a WDS link. Privacy is immediately enabled if anything different from 'none' is selected and an appropriate key has been set. For wep40default(2) or wep104default(3) privacy, the default WEP keys are used, which are shared between all WDS links on a radio module. Enumerations: none (1) wep40 (4) wep104 (5) tkip (6) aes (7)
PrivacyAutoKey
Writing any non-zero value to this attribute triggers automatic bridge privacy setup. Depending on wlanWDSPrivacyMode, a pseudo-random WEP key or passphrase is generated. If non-empty keys have previously been set, writing this attribute has no effect. Reading this attribute always retuns 0. Range: 0 to 1
LinkAliasName
This attribute can be used to set a textual alias name for this bridge link. Default is 'wl?_br?', where first '?' is radio number and second '?' is link number on this radio. Length: 0 to 13
OperStatus
This attribute shows if the bridge link connection is currently operative. Enumerations: true (1) false (2)
DefaultKey
Number of the WEP key to use for encryption of outgoing WDS frames. Enumerations: key1 (1) key2 (2) key3 (3) key4 (4)
Key1
Key string for WEP key nr. 1. Allowed number of octets are 5 for WEP-40 and 13 for WEP-104. Length: 0 to 13
Key2
Key string for WEP key nr. 2. Allowed number of octets are 5 for WEP-40 and 13 for WEP-104. Length: 0 to 13
Key3
Key string for WEP key nr. 3. Allowed number of octets are 5 for WEP-40 and 13 for WEP-104. Length: 0 to 13
Key4
Key string for WEP key nr. 4. Allowed number of octets are 5 for WEP-40 and 13 for WEP-104. Length: 0 to 13
PassPhrase
Passphrase string for WDS encryption type TKIP and AES. Length: 0 to 64
MSDUTx
This attribute counts the total number of packets transmitted on this WDS link.
MSDURx
This attribute counts the total number of packets received on this WDS link.
BytesTx
This attribute counts the total number of octets transmitted on this WDS link.
BytesRx
This attribute counts the total number of octets received on this WDS link.
CurrentRate
This attribute returns the current receive data rate for this link in 500 Kbps units, or 0 if no connection can be established. Range: 0 to 600
CurrentRSSI
This attribute returns the current receive signal strength for this link, or 0 if no connection can be established. Range: -110 to 0
CurrentNoise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established. Range: -110 to 0
TransientKey
Transient key generated from Passphrase string for WDS encryption type TKIP and AES. Length: 16 to 32
LocalAddress
Local MAC Address for the WDS link. Length: 6 to 6
TimeoutCount
This counter increments every second if no packets are received from link partner. If a certain threshold is reached, an ArbopAnnounceLinkUp packet is transmitted in order to resynchronize the bridge partners.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of data frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of data frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of data frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of data frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of data frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of data frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of data frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of data frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of data frames that were received at 1 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFrames48
This attribute shows the number of data frames that were transmitted at 48 Mbps.
TxFrames36
This attribute shows the number of data frames that were transmitted at 36 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames18
This attribute shows the number of data frames that were transmitted at 18 Mbps.
TxFrames12
This attribute shows the number of data frames that were transmitted at 12 Mbps.
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames9
This attribute shows the number of data frames that were transmitted at 9 Mbps.
TxFrames6
This attribute shows the number of data frames that were transmitted at 6 Mbps.
TxFrames5
This attribute shows the number of data frames that were transmitted at 5.5 Mbps.
TxFrames2
This attribute shows the number of data frames that were transmitted at 2 Mbps.
TxFrames1
This attribute shows the number of data frames that were transmitted at 1 Mbps.
CurrentRSSI1
This attribute returns the current receive signal strength on the first receiver for this link, or 0 if no connection can be established. Range: -110 to 0
CurrentRSSI2
This attribute returns the current receive signal strength on the second receiver for this link, or 0 if no second receiver present or no connection can be established. Range: -110 to 0
CurrentRSSI3
This attribute returns the current receive signal strength on the third receiver for this link, or 0 if no third receiver present or no connection can be established. Range: -110 to 0

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH