>> MIB - Management Information Base
>> Table: snmpEngine - (.1.3.6.1.6.3.10.2.1)
snmpEngine
OID | Name | Type | Access
.1 | ID | SnmpEngineID | R
.2 | Boots | INTEGER | R
.3 | Time | INTEGER | R
.4 | MaxMessageSize | INTEGER | R
ID
An SNMP engine's administratively-unique identifier. This information SHOULD be stored in non-volatile storage so that it remains constant across re-initializations of the SNMP engine. Length: 5 to 32
Boots
The number of times that the SNMP engine has (re-)initialized itself since snmpEngineID was last configured. Range: 1 to 2147483647
Time
The number of seconds since the value of the snmpEngineBoots object last changed. When incrementing this object's value would cause it to exceed its maximum, snmpEngineBoots is incremented as if a re-initialization had occurred, and this object's value consequently reverts to zero. Range: 0 to 2147483647
MaxMessageSize
The maximum length in octets of an SNMP message which this SNMP engine can send or receive and process, determined as the minimum of the maximum message size values supported among all of the transports available to and supported by the engine. Range: 484 to 2147483647

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH