>> MIB - Management Information Base
>> Table: pimSGRptITable - (.1.3.6.1.4.1.272.4.5.54.2.1.9.1)
Description: An entry (conceptual row) in the pimSGRptITable.
pimSGRptITable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | UpTime | TimeTicks | R
.3 | LocalMembership | ENUM | R
.4 | JoinPruneState | ENUM | R
.5 | PrunePendingTimer | TimeTicks | R
.6 | PruneExpiryTimer | TimeTicks | R
IfIndex
The ifIndex of the interface that this entry corresponds to. Range: 1 to 2147483647
UpTime
The time since this entry was created by the local router.
LocalMembership
Whether the local router has both (*,G) include local membership and (S,G) exclude local membership on this interface (resulting from a mechanism such as IGMPv3 or MLDv2). This corresponds to local_receiver_exclude(S,G,I) in the PIM-SM specification. Enumerations: true (1) false (2)
JoinPruneState
The state resulting from (S,G,rpt) Join/Prune messages received on this interface. This corresponds to the state of the downstream per-interface (S,G,rpt) state machine in the PIM-SM specification. Enumerations: noInfo (1) prune (2) prunePending (3) pruneTmp (4) prunePendingTmp (5)
PrunePendingTimer
The time remaining before the local router starts pruning this source off the RP tree. This timer is called the (S,G,rpt) Prune-Pending Timer in the PIM-SM specification. This object is zero if the timer is not running.
PruneExpiryTimer
The time remaining before (S,G,rpt) Prune state for this interface expires. This timer is called the (S,G,rpt) Prune Expiry Timer in the PIM-SM specification. This object is zero if the timer is not running. A value of 'FFFFFFFF'h indicates an infinite expiry time.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH