>> MIB - Management Information Base
>> Table: mobileGPSInfoTable - (.1.3.6.1.4.1.272.4.41.4.1.26.1)
Description: A single mobileGPSInfoTable entry.
mobileGPSInfoTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | OperStatus | ENUM | R
.3 | Date | DisplayString | R
.4 | Time | DisplayString | R
.5 | Latitude | DisplayString | R
.6 | Longitude | DisplayString | R
.7 | SpeedOverGround | INTEGER | R
.8 | NumberOfSatelites | INTEGER | R
IfIndex
The index of the corresponding TTY interface.
OperStatus
The operation status of the UMTS modems internal GPS module. The following states can occur: - unknown(1) -- initialization failed - down(2) -- GPS module disabled - init(3) -- GPS module is looking for satelites - up(4) -- GPS module is providing GPS info Enumerations: unknown (1) down (2) init (3) up (4)
Date
The actual date calculated from GPS info. Length: 0 to 16
Time
The actual time calculated from GPS info. Length: 0 to 16
Latitude
The actual Latitude calculated from GPS info. Length: 0 to 32
Longitude
The actual Longitude calculated from GPS info. Length: 0 to 32
SpeedOverGround
The actually detected Speed over Ground. Range: 0 to 65535
NumberOfSatelites
The number of satelites actually found by the GPS module. Range: 0 to 34

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH