>> MIB - Management Information Base
>> Table: mpsDoorIntercomUserTable - (.1.3.6.1.4.1.272.4.53.7.3.1)
Description: This table contains the mode information for each button of a door intercom.
mpsDoorIntercomUserTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | Button | DoorButtonIndex | RW
.3 | Mode | DoorIntercomModeIndex | RW
.4 | AdminStatus | ENUM | D
Index
A unique value for each door intercom. Reference to mpsDoorIntercomIndex. Range: 1 to 10
Button
A reference to mpsDoorIntercomSourceButton. Range: 1 to 4
Mode
Select the active call mode. Range: 1 to 10
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH