>> MIB - Management Information Base
>> Table: hdsl2ShdslEndpointCurrTable - (.1.3.6.1.4.1.272.4.35.1.1.5.1)
Description: An entry in the hdsl2ShdslEndpointCurrTable. Each entry contains status and performance information relating to a single segment endpoint. It is indexed by the ifIndex of the HDSL2/SHDSL line.
hdsl2ShdslEndpointCurrTable
OID | Name | Type | Access
.1 | CurrIfIndex | INTEGER | R
.2 | CurrReceivedBlks | INTEGER | R
.3 | CurrTransmittedBlks | INTEGER | R
.4 | CurrCorrectedBlks | INTEGER | R
.5 | CurrUncorrectBlks | INTEGER | R
.6 | CurrAtn | INTEGER | R
.7 | CurrSnrMgn | INTEGER | R
.8 | CurrStatus | ENUM | R
.9 | ES | Counter | R
.10 | SES | Counter | R
.11 | CRCanomalies | Counter | R
.12 | LOSWS | Counter | R
.13 | UAS | Counter | R
.14 | Curr15MinReceivedBlks | INTEGER | R
.15 | Curr15MinTransmittedBlks | INTEGER | R
.16 | Curr15MinCorrectedBlks | INTEGER | R
.17 | Curr15MinUncorrectBlks | INTEGER | R
.18 | Curr15MinTimeElapsed | INTEGER | R
.19 | Curr15MinES | INTEGER | R
.20 | Curr15MinSES | INTEGER | R
.21 | Curr15MinCRCanomalies | INTEGER | R
.22 | Curr15MinLOSWS | INTEGER | R
.23 | Curr15MinUAS | INTEGER | R
.24 | Curr1DayReceivedBlks | INTEGER | R
.25 | Curr1DayTransmittedBlks | INTEGER | R
.26 | Curr1DayCorrectedBlks | INTEGER | R
.27 | Curr1DayUncorrectBlks | INTEGER | R
.28 | Curr1DayTimeElapsed | INTEGER | R
.29 | Curr1DayES | INTEGER | R
.30 | Curr1DaySES | INTEGER | R
.31 | Curr1DayCRCanomalies | INTEGER | R
.32 | Curr1DayLOSWS | INTEGER | R
.33 | Curr1DayUAS | INTEGER | R
CurrIfIndex
This object specifies the associated interface index of this HDSL2/SHDSL line.
CurrReceivedBlks
Count of all encoded blocks received on this channel since agent reset.
CurrTransmittedBlks
Count of all encoded blocks transmitted on this channel since agent reset.
CurrCorrectedBlks
Count of all blocks received with errors that were corrected since agent reset. These blocks are passed on as good data.
CurrUncorrectBlks
Count of all blocks received with uncorrectable errors since agent reset.
CurrAtn
The current loop attenuation for this endpoint as reported in a Network or Customer Side Performance Status message. Range: -127 to 128
CurrSnrMgn
The current SNR margin for this endpoint as reported in a Status Response/SNR message. Range: -127 to 128
CurrStatus
Contains the current state of the endpoint. This is a bitmap of possible conditions. The various bit positions are: noDefect There no defects on the line. powerBackoff Indicates enhanced Power Backoff. deviceFault Indicates a vendor-dependent diagnostic or self-test fault has been detected. dcContinuityFault Indicates vendor-dependent conditions that interfere with span powering such as short and open circuits. snrMarginAlarm Indicates that the SNR margin has dropped below the alarm threshold. loopAttenuationAlarm Indicates that the loop attenuation exceeds the alarm threshold. (not supported by GlobeSpan !) loswFailureAlarm Indicates a forward LOSW alarm. configInitFailure Endpoint failure during initialization due to paired endpoint not able to support requested configuration. protocolInitFailure Endpoint failure during initialization due to incompatible protocol used by the paired endpoint. noNeighborPresent Endpoint failure during initialization due to no activation sequence detected from paired endpoint. loopbackActive A loopback is currently active at this Segment Endpoint. This is intended to supplement ifOperStatus. Note that there is a 1-1 relationship between the status bits defined in this object and the notification thresholds defined elsewhere in this MIB. Enumerations: noDefect (1) powerBackoff (2) deviceFault (3) dcContinuityFault (4) snrMarginAlarm (5) loswFailureAlarm (7) configInitFailure (8) protocolInitFailure (9) noNeighborPresent (10) loopbackActive (11)
ES
Count of Errored Seconds (ES) on this endpoint since the xU was last restarted.
SES
Count of Severely Errored Seconds (SES) on this endpoint since the xU was last restarted.
CRCanomalies
Count of CRC anomalies on this endpoint since the xU was last restarted.
LOSWS
Count of Loss of Sync Word (LOSW) Seconds on this endpoint since the xU was last restarted.
UAS
Count of Unavailable Seconds (UAS) on this endpoint since the xU was last restarted.
Curr15MinReceivedBlks
Count of all encoded blocks received on this channel within the mandatory 15 minute interval.
Curr15MinTransmittedBlks
Count of all encoded blocks transmitted on this channel within the mandatory 15 minute interval.
Curr15MinCorrectedBlks
Count of all blocks received with errors that were corrected on this channel within the mandatory 15 minute interval.
Curr15MinUncorrectBlks
Count of all blocks received with uncorrectable errors on this channel within the mandatory 15 minute interval.
Curr15MinTimeElapsed
Total elapsed seconds in the current 15-minute interval. Range: 0 to 86399
Curr15MinES
Count of Errored Seconds (ES) in the current 15-minute interval.
Curr15MinSES
Count of Severely Errored Seconds (SES) in the current 15-minute interval.
Curr15MinCRCanomalies
Count of CRC anomalies in the current 15-minute interval.
Curr15MinLOSWS
Count of Loss of Sync Word (LOSW) Seconds in the current 15-minute interval.
Curr15MinUAS
Count of Unavailable Seconds (UAS) in the current 15-minute interval.
Curr1DayReceivedBlks
Count of all encoded blocks received on this channel during the mandatory day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayTransmittedBlks
Count of all encoded blocks transmitted on this channel during the mandatory day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayCorrectedBlks
Count of all blocks received with errors that were corrected on this channel during the mandatory day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayUncorrectBlks
Count of all blocks received with uncorrectable errors on this channel during the mandatory day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayTimeElapsed
Number of seconds that have elapsed since the beginning of the current 1-day interval. Range: 0 to 86399
Curr1DayES
Count of Errored Seconds (ES) during the current day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DaySES
Count of Severely Errored Seconds (SES) during the current day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayCRCanomalies
Count of CRC anomalies during the current day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayLOSWS
Count of Loss of Sync Word (LOSW) Seconds during the current day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.
Curr1DayUAS
Count of Unavailable Seconds (UAS) during the current day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH