>> MIB - Management Information Base
>> Table: wlcWlanIfStatTable - (.1.3.6.1.4.1.272.4.61.1.25.1)
Description: This table contains the current settings and statistics of each WLAN interface.
wlcWlanIfStatTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Channel | INTEGER | R
.3 | SecondaryChannel | INTEGER | R
.4 | Address | MacAddress | R
.5 | Type | ENUM | R
.6 | Band | ENUM | R
.7 | Mode | ENUM | R
.8 | TxPower | INTEGER | R
.9 | FortyMHzOperation | ENUM | R
.10 | ShortGI | ENUM | R
.11 | NoSpatialEnabled | INTEGER | R
.12 | Greenfield | ENUM | R
.13 | TxPackets | Counter32 | R
.14 | TxBytes | Counter32 | R
.15 | TxDropped | Counter32 | R
.16 | RxPackets | Counter32 | R
.17 | RxBytes | Counter32 | R
.18 | RxErrors | Counter32 | R
.19 | Associated | INTEGER | R
.20 | OperState | ENUM | R
Index
Uniqe WLAN interface statistic index.
Channel
Current selected channel of the requested WLAN interface.
SecondaryChannel
Current secondary channel of the requested WLAN interface.
Address
The MAC address of the requested WLAN interface. Length: 6 to 6
Type
The type which is setup for the requested WLAN interface. Enumerations: off (1) access-point (2) client (3) delete (32)
Band
The current operation band of the requested WLAN interface. Enumerations: b24-GHz (1) b5-GHz (2) b58-GHz (3) b24-5-GHz (4)
Mode
The current operation mode of the requested WLAN interface. Enumerations: m802-11b (1) m802-11g (2) m802-11mixed (3) m802-11mixed-long (4) m802-11mixed-short (5) m802-11a (6) m802-11bgn (7) m802-11gn (8) m802-11n (10) m802-11an (11) m802-11abg (12) m802-11abgn (13) m802-11agn (14)
TxPower
The current transmit power of the requested WLAN interface.
FortyMHzOperation
This variable is TRUE if the requested WLAN interface currently operates with 40MHz bandwidth. Enumerations: true (1) false (2)
ShortGI
This variable is TRUE if the short guard interval is currently enabled on the requested WLAN interface. Enumerations: true (1) false (2)
NoSpatialEnabled
Number of enabled spatial stream on the requested WLAN interface.
Greenfield
This variable is TRUE if the green field option is currently enabled on the requested WLAN interface. Enumerations: true (1) false (2)
TxPackets
Number of transmitted packets.
TxBytes
Number of transmitted bytes.
TxDropped
Number of dropped packets in transmit direction.
RxPackets
Number of received packets.
RxBytes
Number of received bytes.
RxErrors
This variable is counting packets that were not received correctly.
Associated
Number of currently associated clients.
OperState
This attribute reflects the operational state of the corresponding WLAN card. 'true' -> radio is enabled, 'false' -> radio is disabled. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH