>> MIB - Management Information Base
>> Table: dot11PrivacyTable - (.1.2.840.10036.1.5.1)
Description: An entry in the dot11PrivacyTable Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PrivacyTable
OID | Name | Type | Access
.1 | PrivacyInvoked | ENUM | RW
.2 | WEPDefaultKeyID | INTEGER | RW
.3 | WEPKeyMappingLength | Unsigned32 | RW
.4 | ExcludeUnencrypted | ENUM | RW
.5 | WEPICVErrorCount | Counter32 | R
.6 | WEPExcludedCount | Counter32 | R
.7 | RSNAEnabled | ENUM | RW
.8 | RSNAPreAuthenticationEnabled | ENUM | RW
PrivacyInvoked
When this attribute is TRUE, it shall indicate that some level of security is invoked for transmitting frames of type Data. For WEP-only clients, the security mechanism used is WEP. For RSNA-capable clients, an additional variable dot11RSNAEnabled indicates whether RSNA is enabled. If dot11RSNAEnabled is FALSE or the MIB variable does not exist, the security mechanism invoked is WEP; if dot11RSNAEnabled is TRUE, RSNA security mechanisms invoked are configured in the dot11RSNAConfigTable. The default value of this attribute shall be FALSE. Enumerations: true (1) false (2)
WEPDefaultKeyID
This attribute shall indicate the use of the first, second, third, or fourth element of the WEPDefaultKeys array when set to values of zero, one, two, or three. The default value of this attribute shall be 0. Range: 0 to 3
WEPKeyMappingLength
The maximum number of tuples that dot11WEPKeyMappings can hold. Range: 10 to -1
ExcludeUnencrypted
When this attribute is true, the STA shall not indicate at the MAC service interface received MSDUs that have the WEP subfield of the Frame Control field equal to zero. When this attribute is false, the STA may accept MSDUs that have the WEP subfield of the Frame Control field equal to zero. The default value of this attribute shall be false. Enumerations: true (1) false (2)
WEPICVErrorCount
This counter shall increment when a frame is received with the WEP subfield of the Frame Control field set to one and the value of the ICV as received in the frame does not match the ICV value that is calculated for the contents of the received frame.
WEPExcludedCount
This counter shall increment when a frame is received with the Protected Frame subfield of the Frame Control field set to zero and the value of dot11ExcludeUnencrypted causes that frame to be discarded.
RSNAEnabled
When this object is set to TRUE, this shall indicate that RSNA is enabled on this entity. The entity will advertise the RSN Information Element in its Beacon and Probe Response frames. Configuration variables for RSNA operation are found in the dot11RSNAConfigTable. This object requires that dot11PrivacyInvoked also be set to TRUE. Enumerations: true (1) false (2)
RSNAPreAuthenticationEnabled
When this object is set to TRUE, this shall indicate that RSNA preauthentication is enabled on this entity. This object requires that dot11RSNAEnabled also be set to TRUE. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH