>> MIB - Management Information Base
>> Table: ipsecSaTable - (.1.3.6.1.4.1.272.4.26.3.1)
Description: This object contains an IPSec security association.
ipsecSaTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.3 | State | ENUM | R
.5 | Dir | ENUM | R
.6 | Mode | ENUM | R
.7 | SecProto | ENUM | R
.17 | Spi | HexValue | R
.18 | AuthAlg | ENUM | R
.19 | EncAlg | ENUM | R
.20 | CompAlg | ENUM | R
.21 | AuthKeyLen | INTEGER | R
.22 | EncKeyLen | INTEGER | R
.33 | ReplayErrors | INTEGER | R
.34 | RecvErrors | INTEGER | R
.35 | DecryptErrors | INTEGER | R
.39 | Bundle | INTEGER | R
.40 | BundleNesting | INTEGER | R
.45 | SpiSize | INTEGER | R
.64 | EncKey | OCTET STRING | N
.65 | AuthKey | OCTET STRING | N
.66 | IkeMajVersion | INTEGER | R
.67 | IkeMinVersion | INTEGER | R
Index
A unique index for this entry.
State
The current state of the security association Possible values: alive(1), -- The SA is alive expired(2), -- The SA is expired negotiating(4),-- This SA is currently negotiated established(5) -- The SA is alive and will eventually be rekeyed. Enumerations: expired (2) negotiating (4) established (5)
Dir
This object specifies whether the SA is used for inbound or outbound processing. Possible values: inbound(1), -- An inbound security association outbound(2) -- An outbound security association. Enumerations: inbound (1) outbound (2)
Mode
This object specifies whether the SA is in tunnel or transport mode. Possible values: tunnel(1), -- A tunnel mode SA transport(2) -- A transport mode SA. Enumerations: tunnel (1) transport (2)
SecProto
This object specifies the security protocol applied by this SA. Possible values: esp(50), -- Encapsulating Security Payload ah(51), -- Authentication Header ipcomp(108) -- Internet Payload Compression Protocol. Enumerations: esp (50) ah (51) ipcomp (108)
Spi
The Security Parameters Index of this SA. Range: 0 to -1
AuthAlg
The hash algorithm used, if any. Possible Values: none(2), -- No hash algorithm applied md5-96(4), -- The MD5 hash algorithm sha1-96(6) -- The Secure Hash Algorithm. Enumerations: none (2) md5-96 (4) sha1-96 (6)
EncAlg
The encryption algorithm used, if any. Possible Values: none(1), -- No encryption applied des-cbc(2), -- DES in CBC mode des3-cbc(3), -- Triple DES in CBC mode blowfish-cbc(4), -- Blowfish in CBC mode cast128-cbc(5), -- CAST with 128 bit key in CBC mode twofish-cbc(6), -- Twofish in CBC mode aes-cbc(7) -- AES in CBC mode. Enumerations: none (1) des-cbc (2) des3-cbc (3) blowfish-cbc (4) cast128-cbc (5) twofish-cbc (6) aes-cbc (7)
CompAlg
The compression algorithm used, if any. Possible Values: none(1), -- No compression deflate(2) -- DEFLATE compression algorithm. Enumerations: none (2) deflate (3)
AuthKeyLen
The length in bytes of the key used for authentication, if any.
EncKeyLen
The length in bytes of the key used for encryption, if any.
ReplayErrors
The number of replayed packets detected for this SA.
RecvErrors
The number of receive errors (replayed packets not counted) detected for this SA.
DecryptErrors
The number of decryption errors (ESP only) detected for this SA.
Bundle
unique id of SA-bundle within this SA is used.
BundleNesting
place of SA within SA-Bundle.
SpiSize
The size of the SPI in bytes.
EncKey
description not available
AuthKey
description not available
IkeMajVersion
The IKE major version number.
IkeMinVersion
The IKE minor version number.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH