>> MIB - Management Information Base
>> Table: mobileOperatorTable - (.1.3.6.1.4.1.272.4.41.4.1.23.1)
Description: A single mobileOperatorTable entry.
mobileOperatorTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Code | INTEGER | R
.3 | AcT | ENUM | R
.4 | Status | ENUM | R
.5 | Name | DisplayString | R
.6 | Priority | INTEGER | R
.7 | Preference | ENUM | R
.8 | CurrentOrder | INTEGER | R
IfIndex
The index of the corresponding TTY interface.
Code
The PLMN code of the network operator.
AcT
The Access Type the modem actually registers on. Normally the `edge' or `hs*pa' Access Types aren't provided in detail by the network operator and/or modem. Possible Access Types are: unknown(1) gsm(2) -- GSM compact-gsm(3) -- CGSM umts(4) -- UMTS gsm-edge(5) -- GPRS/EDGE umts-hsdpa(6) -- HSDPA umts-hsupa(7) -- HSUPA umts-hspa(8) -- HSPA lte(9) -- LTE hspa-plus(10) -- HSPA+ cdma-rev0(11) -- CDMA 1xEV-DO Rev. 0 cdma-revA(12) -- CDMA 1xEV-DO Rev. A cdma-revB(13) -- CDMA 1xEV-DO Rev. B Enumerations: unknown (1) gsm (2) compact-gsm (3) umts (4) gsm-edge (5) umts-hsdpa (6) umts-hsupa (7) umts-hspa (8) lte (9) hspa-plus (10) cdma-rev0 (11) cdma-revA (12) cdma-revB (13)
Status
The registration status depending on the network operator. The following states can occur: - unknown(1) -- no idea - available(2) -- registration possible - current(3) -- successfully registered - forbidden(4) -- no roaming possible Enumerations: unknown (1) available (2) forbidden (4)
Name
The name of the network operator. Length: 0 to 60
Priority
The Priority of the Operator to use in roaming mode. There are different priority value ranges for the following types of operator entries: - Home Operator (from SIM card) - Priviledged Operator (from SIM card) - Administrative Operator - Preferred Operator - Practicable Operator The start and the size of each priority range is predefined but variable and will be configurable in future via the global mobile settings.
Preference
The registration priority for the network operator. The following states can occur: - home(1) -- home operator - privileged(2) -- home operators best roaming partner - preferred(3) -- home operators roaming partner - practicable(4) -- roaming possible but not preferred - banned(5) -- no roaming to this operator possible - administrative(6) -- configured via mobileAdmOperatorTable Enumerations: home (1) privileged (2) preferred (3) practicable (4) banned (5) administrative (6)
CurrentOrder
The order of the entry in the currently used internal roaming list, the value '-1' indicates an unused (ignored) entry.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH