>> MIB - Management Information Base
>> Table: upnpIfTable - (.1.3.6.1.4.1.272.4.5.45.30.10)
Description: An entry in the upnpIfTable.
upnpIfTable
OID | Name | Type | Access
.10 | Index | INTEGER | R
.20 | ClientRequests | ENUM | RW
.30 | UPnPControlled | ENUM | RW
Index
This object specifies the interface index, for which the table entry shall be valid.
ClientRequests
This object specifies whether UPnP accepts client requests received through this interface. Possible values: enabled(10) -- UPnP client requests enabled disabled(20) -- UPnP client requests disabled (default). Enumerations: enabled (10) disabled (20)
UPnPControlled
This object specifies if this interface can be controlled through UPnP requests. Possible values: enabled(10) -- UPnP control of the interface enabled disabled(20) -- UPnP control of the interface disabled (default). Enumerations: enabled (10) disabled (20)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH