>> MIB - Management Information Base
>> Table: dot11PhyDSSSTable - (.1.2.840.10036.4.5.1)
Description: An entry in the dot11PhyDSSSEntry Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyDSSSTable
OID | Name | Type | Access
.1 | CurrentChannel | INTEGER | RW
.2 | CCAModeSupported | INTEGER | R
.3 | CurrentCCAMode | ENUM | RW
.4 | EDThreshold | Integer32 | RW
CurrentChannel
The current operating frequency channel of the DSSS PHY. Valid channel numbers are as defined in 15.4.6.2 Range: 1 to 14
CCAModeSupported
dot11CCAModeSupported is a bit-significant value, representing all of the CCA modes supported by the PHY. Valid values are: energy detect only (ED-ONLY) = 01, carrier sense only (CS-ONLY) = 02, carrier sense and energy detect (ED-and-CS)= 04 or the logical sum of any of these values. This attribute shall not be used to indicate the CCA modes supported by a higher rate extension PHY. Rather, the dot11HRCCAModeSupported attribute shall be used to indicate the CCA modes of the higher rate extension PHY. Range: 1 to 7
CurrentCCAMode
The current CCA method in operation. Valid values are: energy detect only (edonly) = 01, carrier sense only (csonly) = 02, carrier sense and energy detect (edandcs)= 04. carrier sense with timer (cswithtimer)= 08 high rate carrier sense and energy detect (hrcsanded)= 16 Enumerations: edonly (1) csonly (2) edandcs (4) cswithtimer (8) hrcsanded (16)
EDThreshold
The current Energy Detect Threshold being used by the DSSS PHY.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH