>> MIB - Management Information Base
>> Table: atmAtucPerfDataTable - (.1.3.6.1.4.1.272.4.16.21.1)
Description: An entry in atmAtucPerfDataTable.
atmAtucPerfDataTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | IdleCells | INTEGER | R
.3 | DataCells | INTEGER | R
.4 | Lcds | INTEGER | R
.5 | Hecs | INTEGER | R
.11 | Curr15MinTimeElapsed | INTEGER | R
.12 | Curr15MinIdleCells | INTEGER | R
.13 | Curr15MinDataCells | INTEGER | R
.14 | Curr15MinLcds | INTEGER | R
.15 | Curr15MinHecs | INTEGER | R
.18 | Curr1DayTimeElapsed | INTEGER | R
.19 | Curr1DayIdleCells | INTEGER | R
.20 | Curr1DayDataCells | INTEGER | R
.21 | Curr1DayLcds | INTEGER | R
.22 | Curr1DayHecs | INTEGER | R
.26 | Prev1DayIdleCells | INTEGER | R
.27 | Prev1DayDataCells | INTEGER | R
.28 | Prev1DayLcds | INTEGER | R
.29 | Prev1DayHecs | INTEGER | R
IfIndex
Specifies the ATM interface index.
IdleCells
The number of ATM idle cells.
DataCells
The number of ATM data cells.
Lcds
Count of the number of Loss of Cell Delineation failures since agent reset.
Hecs
Count of the number of Header Error Check failures since agent reset.
Curr15MinTimeElapsed
Total elapsed seconds in this interval. Range: 0 to 899
Curr15MinIdleCells
The number of ATM idle cells in the mandatory 15 minute interval.
Curr15MinDataCells
The number of ATM data cells in the mandatory 15 minute interval.
Curr15MinLcds
Count of seconds in the mandatory 15 minute interval when there was Loss of Cell Delineation.
Curr15MinHecs
Count of seconds in the mandatory 15 minute interval when there was Header Error Check failures.
Curr1DayTimeElapsed
Number of seconds that have elapsed since the beginning of the mandatory 1-day interval. Range: 0 to 86399
Curr1DayIdleCells
The number of ATM idle cells during the mandatory day as measured by atmAtucPerfCurr1DayTimeElapsed.
Curr1DayDataCells
The number of ATM data cells during the mandatory day as measured by atmAtucPerfCurr1DayTimeElapsed.
Curr1DayLcds
Count of the number of seconds when there was Loss of Cell Delineation during the mandatory day as measured by atmAtucPerfCurr1DayTimeElapsed.
Curr1DayHecs
Count of the number of seconds when there was Header Error Check failures during the mandatory day as measured by atmAtucPerfCurr1DayTimeElapsed.
Prev1DayIdleCells
The number of ATM idle cells within the most recent previous 1-day period.
Prev1DayDataCells
The number of ATM data cells within the most recent previous 1-day period.
Prev1DayLcds
Count of seconds in the interval when there was Loss of Cell Delineation within the most recent previous 1-day period.
Prev1DayHecs
Count of seconds in the interval when there was Header Error Check within the most recent previous 1-day period.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH