>> MIB - Management Information Base
>> Table: adslAtucChanPerfDataTable - (.1.3.6.1.4.1.272.4.30.1.1.13.1)
Description: An entry in adslAtucChanPerfDataTable.
adslAtucChanPerfDataTable
OID | Name | Type | Access
.1 | PerfIfIndex | INTEGER | R
.2 | ReceivedBlks | INTEGER | R
.3 | TransmittedBlks | INTEGER | R
.4 | CorrectedBlks | INTEGER | R
.5 | UncorrectBlks | INTEGER | R
.6 | PerfValidIntervals | INTEGER | R
.7 | PerfInvalidIntervals | INTEGER | R
.8 | PerfCurr15MinTimeElapsed | INTEGER | R
.9 | PerfCurr15MinReceivedBlks | INTEGER | R
.10 | PerfCurr15MinTransmittedBlks | INTEGER | R
.11 | PerfCurr15MinCorrectedBlks | INTEGER | R
.12 | PerfCurr15MinUncorrectBlks | INTEGER | R
.13 | PerfCurr1DayTimeElapsed | INTEGER | R
.14 | PerfCurr1DayReceivedBlks | INTEGER | R
.15 | PerfCurr1DayTransmittedBlks | INTEGER | R
.16 | PerfCurr1DayCorrectedBlks | INTEGER | R
.17 | PerfCurr1DayUncorrectBlks | INTEGER | R
.18 | PerfPrev1DayMoniSecs | INTEGER | R
.19 | PerfPrev1DayReceivedBlks | INTEGER | R
.20 | PerfPrev1DayTransmittedBlks | INTEGER | R
.21 | PerfPrev1DayCorrectedBlks | INTEGER | R
.22 | PerfPrev1DayUncorrectBlks | INTEGER | R
PerfIfIndex
Specifies the ADSL interface index.
ReceivedBlks
Count of all encoded blocks received on this channel since agent reset.
TransmittedBlks
Count of all encoded blocks transmitted on this channel since agent reset.
CorrectedBlks
Count of all blocks received with errors that were corrected since agent reset. These blocks are passed on as good data.
UncorrectBlks
Count of all blocks received with uncorrectable errors since agent reset.
PerfValidIntervals
The number of previous 15-minute intervals in the interval table for which data was collected. Given that <n> is the maximum # of intervals supported. The value will be <n> unless the measurement was (re-)started within the last (<n>*15) minutes, in which case the value will be the number of complete 15 minute intervals for which the agent has at least some data. In certain cases (e.g., in the case where the agent is a proxy) it is possible that some intervals are unavailable. In this case, this interval is the maximum interval number for which data is available. Range: 0 to 96
PerfInvalidIntervals
The number of intervals in the range from 0 to the value of adslAtucChanPerfValidIntervals for which no data is available. This object will typically be zero except in cases where the data for some intervals are not available (e.g., in proxy situations). Range: 0 to 96
PerfCurr15MinTimeElapsed
Total elapsed seconds in this interval. A full interval is 900 seconds. Range: 0 to 899
PerfCurr15MinReceivedBlks
Count of all encoded blocks received on this channel within the mandatory 15 minute interval.
PerfCurr15MinTransmittedBlks
Count of all encoded blocks transmitted on this channel within the mandatory 15 minute interval.
PerfCurr15MinCorrectedBlks
Count of all blocks received with errors that were corrected on this channel within the mandatory 15 minute interval.
PerfCurr15MinUncorrectBlks
Count of all blocks received with uncorrectable errors on this channel within the mandatory 15 minute interval.
PerfCurr1DayTimeElapsed
Number of seconds that have elapsed since the beginning of the mandatory 1-day interval. Range: 0 to 86399
PerfCurr1DayReceivedBlks
Count of all encoded blocks received on this channel during the mandatory day as measured by adslAtucChanPerfCurr1DayTimeElapsed.
PerfCurr1DayTransmittedBlks
Count of all encoded blocks transmitted on this channel during the mandatory day as measured by adslAtucChanPerfCurr1DayTimeElapsed.
PerfCurr1DayCorrectedBlks
Count of all blocks received with errors that were corrected on this channel during the mandatory day as measured by adslAtucChanPerfCurr1DayTimeElapsed.
PerfCurr1DayUncorrectBlks
Count of all blocks received with uncorrectable errors on this channel during the mandatory day as measured by adslAtucChanPerfCurr1DayTimeElapsed.
PerfPrev1DayMoniSecs
The amount of time in the previous 1-day interval over which the performance monitoring information is actually counted. This value will be the same as the interval duration except in a situation where performance monitoring data could not be collected for any reason. Range: 0 to 86400
PerfPrev1DayReceivedBlks
Count of all encoded blocks received on this channel within the most recent previous 1-day period.
PerfPrev1DayTransmittedBlks
Count of all encoded blocks transmitted on this channel within the most recent previous 1-day period.
PerfPrev1DayCorrectedBlks
Count of all blocks received with errors that were corrected on this channel within the most recent previous 1-day period.
PerfPrev1DayUncorrectBlks
Count of all blocks received with uncorrectable errors on this channel within the most recent previous 1-day period.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH