>> MIB - Management Information Base
>> Table: vmsAccountUserTable - (.1.3.6.1.4.1.272.4.34.1.4.1)
Description: This table lists the Voice Account User configured for VMS call redirect.
vmsAccountUserTable
OID | Name | Type | Access
.1 | Index | AccountIndex | RW
.2 | Pin | DisplayString | RW
.3 | Mode | ENUM | RW
.4 | Facilities | BITS | RW
.5 | BusinessType | ENUM | RW
.6 | OutBusinessType | ENUM | RW
.7 | AdminStatus | ENUM | D
.8 | Notify | ENUM | RW
Index
A unique value for each Account User Entry. Range: 1 to 65535
Pin
PIN for access to this account. If no PIN defined, then use PIN from mpsUserTable. Length: 0 to 255
Mode
This value contains the active mode of the voice box. It simply chooses the announcement type the VMS shall use. This item can be changed by several means, for instance calendar or web user portal. Enumerations: business (1) outsideBusiness (2)
Facilities
Facility settings for the VMS account: pin-less-access: no PIN check for call of voice box owner. file-move-after-email: new messages are moved to old folder after email notification file-delete-after-email: delete file after successful email notification Enumerations: pin-less-access (0) file-move-after-email (1) file-delete-after-email (2)
BusinessType
Voice Box usage within business time. annOnly: Announcement only (infobox) annAndRec: Announcement and recording Enumerations: annOnly (1) annAndRec (2)
OutBusinessType
Voice box usage outside business time. annOnly: Announcement only (infobox) annAndRec: Announcement and recording Enumerations: annOnly (1) annAndRec (2)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
Notify
Specifies the (user) mail notification mode: no(1) : no mail is sent mail(2) : send a mail without attachment mail-attachment(3): send a mail with the new message attached Enumerations: no (1) mail (2) mail-attachment (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH