>> MIB - Management Information Base
>> Table: isdnCreditsTable - (.1.3.6.1.4.1.272.4.2.12.1)
Description: The isdnCreditsTable contains informations about current used resources and maximum allowed resources for each during a specified interval subsystem. Creating entries: Entries are added by the system during startup. Deleting entries: Is not possible.
isdnCreditsTable
OID | Name | Type | Access
.1 | SubsysNumber | ENUM | R
.2 | Surveillance | ENUM | RW
.3 | Measuretime | INTEGER | RW
.4 | MaxInCon | INTEGER | RW
.5 | MaxOutCon | INTEGER | RW
.6 | MaxCharge | INTEGER | RW
.7 | MaxInDuration | INTEGER | RW
.8 | MaxOutDuration | INTEGER | RW
.9 | Timeleft | INTEGER | RW
.10 | CurrentInCon | INTEGER | R
.11 | CurrentOutCon | INTEGER | R
.12 | TotalInCon | INTEGER | R
.13 | TotalOutCon | INTEGER | R
.14 | TotalMaxCon | INTEGER | R
.15 | TotalCharge | INTEGER | R
.16 | TotalInDuration | INTEGER | R
.17 | TotalOutDuration | INTEGER | R
.18 | MaxCurrentInCon | INTEGER | RW
.19 | MaxCurrentOutCon | INTEGER | RW
.20 | MaxCurrentCon | INTEGER | RW
SubsysNumber
Type of Subsystem. Enumerations: ppp (1) capi (2) isdnlogin (3) pots (4) doorintercom (5)
Surveillance
Surveillance on or off. Enumerations: off (1) on (2)
Measuretime
Time of one observation interval in seconds.
MaxInCon
Maximum number of allowed incoming connections during the observation interval. -1 disables this limit.
MaxOutCon
Maximum number of allowed outgoing connections during the observation interval. -1 disables this limit.
MaxCharge
Maximum allowed charge amount during the observation interval. -1 disables this limit.
MaxInDuration
Maximum connect time for incoming connections in seconds during the observation interval. -1 disables this limit.
MaxOutDuration
Maximum connect time for outgoing connections in seconds during the observation interval. -1 disables this limit
Timeleft
Time in seconds left in current interval. Writing to Timeleft will restart the observation interval.
CurrentInCon
Current number of incoming connections.
CurrentOutCon
Current number of outgoing connections.
TotalInCon
Total count of incoming connections during the observation interval.
TotalOutCon
Total count of outgoing connections during the observation interval.
TotalMaxCon
Maximum number of simultaniously established connections during the observation interval.
TotalCharge
Total accounted charge during the observation interval.
TotalInDuration
Total connect time of incoming connections during the observation interval.
TotalOutDuration
Total connect time of outgoing connections during the observation interval.
MaxCurrentInCon
Maximum number of currently allowed incoming connections. -1 disables this limit.
MaxCurrentOutCon
Maximum number of currently allowed outgoing connections. -1 disables this limit.
MaxCurrentCon
Maximum number of currently allowed connections in both directions. -1 disables this limit.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH