>> MIB - Management Information Base
>> Table: mpsDeviceTable - (.1.3.6.1.4.1.272.4.53.3.1.1)
Description: This table contains information about each call control interface (device internal and external).
mpsDeviceTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RW
.2 | Mode | ENUM | RW
.3 | DisplayName | DisplayString | RW
.4 | Bundle | INTEGER | RW
.5 | TrunkGroup | TrunkGroupIndexOrZero | RW
.6 | DefaultExtension | ExtensionIndexOrZero | RW
.7 | BusMode | ENUM | RW
.8 | ClipNoScreening | ENUM | RW
.9 | AdminStatus | ENUM | D
.10 | Layer2AlwaysOn | ENUM | RW
.11 | Type | ENUM | RW
IfIndex
A unique value for each device. Range: 1 to 2147483647
Mode
Contains mode of the device. itrunk-pmp(2) : isdn extern, point-to-multipoint itrunk-pp(3) : isdn extern, point-to-point iline-pmp(4) : isdn intern, point-to-multipoint iline-pp(5) : isdn intern, point-to-point analine(6) : analoque intern, FXS itrunk-pp-S2m(7): isdn extern, primary rate interfaces dectline(8) : dect intern anatrunk(9) : analoque extern, FXO Enumerations: none (1) itrunk-pmp (2) itrunk-pp (3) iline-pmp (4) iline-pp (5) analine (6) itrunk-pp-S2m (7) dectline (8) anatrunk (9)
DisplayName
Display name of the device. Length: 0 to 32
Bundle
This variable contains the bundle number of the device.
TrunkGroup
A unique value for each trunk group index (reference to mpsTrunkGroupTable). Range: 0 to 65535
DefaultExtension
Defines the extension to be used for outgoing calls without calling party number (reference to mpsExtensionTable). Range: 0 to 65535
BusMode
The configuration of the internal isdn device port is standard(1) or extended(2) Enumerations: standard (1) extended (2)
ClipNoScreening
This value determine when the mpsDeviceMode = itrunk-pp, wether ClipNoScreening is disabled(1) or individual(2) or global(3). Enumerations: no (1) individual (2) global (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2) disable (3)
Layer2AlwaysOn
This value determine if the Layer2 for this external isdn port is keept permanently active (true) or not (false). Enumerations: true (1) false (2)
Type
Set to 'tdm' for physical interfaces (isdn, pots) and set to 'ip' or 'capi' for virtual interfaces. Enumerations: tdm (1) ip (2) capi (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH