>> MIB - Management Information Base
>> Table: tr069WANDeviceXrefTable - (.1.3.6.1.4.1.272.4.22.6.2.9.1)
Description: An entry containing a cross reference between a WANDevice and associated local table entries.
tr069WANDeviceXrefTable
OID | Name | Type | Access
.1 | DeviceIdx | INTEGER | RW
.2 | DeviceATMIfIndex | INTEGER | RW
.3 | ConnectionDeviceIdx | INTEGER | RW
.4 | ConnectionDeviceType | ENUM | D
.5 | ConnectionDeviceIfIndex | INTEGER | RW
.6 | ConnectionDeviceIfType | ENUM | RW
.7 | PPPConnectionIdx | INTEGER | RW
.8 | PPPIfIndex | INTEGER | RW
.9 | XMLTreeState | ENUM | RW
.10 | IPConnectionIdx | INTEGER | RW
DeviceIdx
Index of this WAN device as represented to TR-069.
DeviceATMIfIndex
ATM Interface for this Device.
ConnectionDeviceIdx
Index of this WANConnectionDevice as represented to TR-069. Range: 0 to 2147483647
ConnectionDeviceType
Type of this WANConnectionDevice. Enumerations: pPPoE (1) pPPoA (2) iPoA (3) unconfigured (4) delete (5)
ConnectionDeviceIfIndex
Index of the interface for this WANConnectionDevice.
ConnectionDeviceIfType
Type of the interface associated with this WANConnectionDevice. Enumerations: ethoa (1) pppoa (2) rpoa (3) undefined (4)
PPPConnectionIdx
Index of this PPP connection as represented to TR-069.
PPPIfIndex
Index of this PPP interface.
XMLTreeState
Whether this entry is present in the XML tree. Enumerations: setup (1) new (2) present (3) purge (4)
IPConnectionIdx
Index of this IP connection as represented to TR-069.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH