>> MIB - Management Information Base
>> Table: biboPPPIpAssignTable - (.1.3.6.1.4.1.272.4.3.4.1)
Description: Pool of IP addresses for dynamic IP address assignment via IPCP. See the biboPPPIpAddress field for further explanation.
biboPPPIpAssignTable
OID | Name | Type | Access
.1 | Address | IpAddress | RW
.2 | State | ENUM | D
.3 | PoolId | INTEGER | RW
.4 | Range | INTEGER | RW
.5 | Description | DisplayString | RW
Address
First IP address of this range.
State
If an entry is currently in use, the state is set to as- signed(1). Otherwise it is set to unused(2). You may also delete this entry by changing it to delete(3). Enumerations: unused (1) assigned (2) delete (3)
PoolId
Pool ID value.
Range
Number of IP addresses that will be assigned starting from biboPPPIpAssignAddress. A range of 0 will disable this entry
Description
Optional IP pool description. Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH