>> MIB - Management Information Base
>> Table: atmVccTable - (.1.3.6.1.4.1.272.4.16.12.1)
Description: An entry in the table, containing information about a particular virtual channel connection.
atmVccTable
OID | Name | Type | Access
.1 | PortIndex | INTEGER | R
.2 | Vpi | INTEGER | R
.3 | Vci | INTEGER | R
.4 | OperStatus | ENUM | R
PortIndex
The interface index of the associated ATM hardware.
Vpi
The VPI value of this Virtual Channel Connection. Range: 0 to 255
Vci
The VCI value of this Virtual Channel Connection. Range: 0 to 65535
OperStatus
The present actual operational status of the VCC. A value of end2endUp(2) or end2endUp(3) is used if the end-to-end status is known. If only local status is known a value of localUpEnd2endUnknown(4) or localDown(5) is used. Enumerations: unknown (1) end2endUp (2) end2endDown (3) localUpEnd2endUnknown (4) localDown (5)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH